faultsfaults
Metadata also available as
Metadata:
  Identification_Information 
  Data_Quality_Information 
  Spatial_Data_Organization_Information 
  Spatial_Reference_Information 
  Entity_and_Attribute_Information 
  Distribution_Information 
  Metadata_Reference_Information 



  Identification_Information: 
    Citation: 
      Citation_Information: 
        Originator: Sandra Troutman 
        Publication_Date: 01/03 
        Title: faults 
        Geospatial_Data_Presentation_Form: vector digital data 
        Online_Linkage: 
        
\\MARINE15058\D$\workspace\coverages\final_open_file\all_files\expanded_files\fa
ults 

    Description: 
      Abstract: 
      This digital map database represents the general distribution of major 
      structures, lithologic contacts, faults, folds and gravity anomalies in 
      the state of Alaska and dominant movement along these faults. This 
      coverage is a digital version of linework from the previously published 
      map, Map showing sedimentary basins of onshore and continental shelf 
      areas, Alaska, C. E. Kirschner (1988). The scale of the source map limits 
      the spatial resolution (scale) of the database to 1:2,500,000 or smaller. 
      Purpose: 
      This database depicts the distribution of major structures, faults, folds 
      and gravity anomalies in the state of Alaska as shown on C. E. 
      Kirschner's, Map showing sedimentary basins of onshore and continental 
      shelf areas, Alaska (1988). This coverage includes linear features only, 
      with polygon features included in an accompanying coverage. The regional 
      (1:2,500,000) scale of this coverage does not provide sufficient detail 
      for site development purposes and this map does not take the place of 
      fault-rupture hazard zone maps. Similarly, the database cannot be 
      substituted for comprehensive maps that systematically identify and 
      classify active fault movement. This coverage is intended for use as a 
      base map for the accompanying open-file report "Map and digital database 
      of sedimentary basins and indications of petroleum in the Central Alaska 
      Province." 
      Supplemental_Information: 
      This database was digitized from previously published data and was 
      compiled in ArcInfo, a commercial Geographic Information System 
      (Environmental Systems Research Institute, Redlands, California), version 
      8.2.0. The files are coverage (ArcInfo vector data) format. Coverages are 
      stored in uncompressed ARC export format (ArcInfo version 8.2.0). ArcInfo 
      export files (files with .e00 extensions) can be converted into ArcInfo 
      coverages in ArcInfo and can be read by some other Geographic Information 
      Systems, such as MapInfo and ESRI's ArcView (limited versions of this 
      software are available for free from ESRI's web site: 
      <http://www.esri.com>). 
    Time_Period_of_Content: 
      Time_Period_Information: 
        Single_Date/Time: 
          Calendar_Date: 2002 
      Currentness_Reference: publication date 
    Status: 
      Progress: Complete 
      Maintenance_and_Update_Frequency: None planned 
    Spatial_Domain: 
      Bounding_Coordinates: 
        West_Bounding_Coordinate: -179.991747 
        East_Bounding_Coordinate: 179.985246 
        North_Bounding_Coordinate: 73.247353 
        South_Bounding_Coordinate: 50.101174 
    Keywords: 
      Theme: 
        Theme_Keyword_Thesaurus: 
        REQUIRED: Reference to a formally registered thesaurus or a similar 
        authoritative source of theme keywords. 
        Theme_Keyword: faults 
        Theme_Keyword: major faults 
        Theme_Keyword: Alaska faults 
        Theme_Keyword: Alaska geology 
        Theme_Keyword: structural geology 
        Theme_Keyword: geologic structure 
        Theme_Keyword: geology 
        Theme_Keyword: gravity 
        Theme_Keyword: gravity anomoly 
      Place: 
        Place_Keyword: Alaska 
        Place_Keyword: United States of America 
      Stratum: 
        Stratum_Keyword: gravity high 
        Stratum_Keyword: gravity low 
        Stratum_Keyword: Bouguer gravity 
        Stratum_Keyword: Bruin Bay fault zone 
        Stratum_Keyword: Castle Mountain fault zone 
        Stratum_Keyword: Chatham Strait fault zone 
        Stratum_Keyword: Contact fault zone 
        Stratum_Keyword: Denali fault zone 
        Stratum_Keyword: Eagle River fault zone 
        Stratum_Keyword: Fairweather fault zone 
        Stratum_Keyword: Farwell fault zone 
        Stratum_Keyword: Iditarod fault zone 
        Stratum_Keyword: Kaltag fault zone 
        Stratum_Keyword: Kobuk fault zone 
        Stratum_Keyword: Kodiak shelf 
        Stratum_Keyword: Middleton Yakataga thrust belt 
        Stratum_Keyword: Mulchatna fault zone 
        Stratum_Keyword: Ruby Rampart trough 
        Stratum_Keyword: Selawik trough 
        Stratum_Keyword: Tintina fault zone 
        Stratum_Keyword: Transition fault zone 
    Access_Constraints: none 
    Use_Constraints: 
    Uses of this digital coverage should not violate the spatial resolution of 
    the data. Although the digital form of the data removes the constraint 
    imposed by the scale of a paper map, the detail and accuracy inherent in map 
    scale are also present in the digital data. The fact that this database was 
    edited for a scale of 1:2,500,000 means that higher resolution information 
    is not present in the dataset. Plotting at scales larger than 1:2,500,000 
    will not yield greater real detail, although it may reveal fine-scale 
    irregularities below the intended resolution of the database 
    Point_of_Contact: 
      Contact_Information: 
        Contact_Person_Primary: 
          Contact_Person: Sandra Troutman 
          Contact_Organization: USGS, Menlo Park, CA 
        Contact_Position: GIS Specialist 
        Contact_Voice_Telephone: 650-329-4974 
        Contact_Facsimile_Telephone: 650-329-4975 
        Contact_Electronic_Mail_Address: stroutman@usgs.gov 
        Hours_of_Service: business hours PST 
    Data_Set_Credit: Sandra Troutman 
    Security_Information: 
      Security_Classification_System: none 
      Security_Classification: Unclassified 
      Security_Handling_Description: none 
    Native_Data_Set_Environment: 
    Microsoft Windows 2000 Version 5.0 (Build 2195) Service Pack 1; ESRI 
    ArcCatalog 8.2.0.700 



  Data_Quality_Information: 
    Logical_Consistency_Report: 
    All features in the dataset were digitized from the same georeferenced, 
    paper map. Therefore, spatial errors within the dataset associated with 
    geoferencing are internally consistent. 
    Completeness_Report: 
    This dataset is intended to describe completely the major linear structures 
    located on the source map as cited. 
    Lineage: 
      Source_Information: 
        Source_Citation: 
          Citation_Information: 
            Originator: C. E. Kirschner 
            Publication_Date: 1988 
            Title: 
            Map showing sedimentary basins of onshore and continental shelf 
            areas, Alaska 
            Series_Information: 
              Series_Name: Miscellaneous Investigations Series 
              Issue_Identification: I-1873 
            Publication_Information: 
              Publisher: United States Geological Survey 
        Source_Scale_Denominator: 1:2,500,000 
        Type_of_Source_Media: Paper map 
        Source_Time_Period_of_Content: 
          Time_Period_Information: 
            Single_Date/Time: 
              Calendar_Date: 1988 
          Source_Currentness_Reference: publication date 
        Source_Citation_Abbreviation: 
        C. E. Kirschner, Map showing sedimentary basins of onshore and 
        continental shelf areas, Alaska, 1988. 
        Source_Contribution: All line features were digitized from this source 
      Process_Step: 
        Process_Description: 
        This database was digitized from previously published data. The geologic 
        map information was digitized from stable originals of the sedimentary 
        basins map at a scale of 1:2,500,000. The author's paper map was scanned 
        on a large-scale, flatbed, color scanner with a resolution of 600 dots 
        per inch. The scanned image was georeferenced interactively to a USGS 
        coverage of the state of Alaska using ArcInfo georeferencing software 
        and rectified with a first order polynomial transformation. The line 
        features were digitized interactively by hand using ArcInfo. 
        Process_Date: 2002 
        Process_Contact: 
          Contact_Information: 
            Contact_Person_Primary: 
              Contact_Person: Sandra Troutman 
              Contact_Organization: US Geolgocial Survey 
            Contact_Position: GIS Specialist 
            Contact_Address: 
              Address_Type: mailing address 
              Address: 345 Middlefield Road MS 969 
              City: Menlo Park 
              State_or_Province: California 
              Postal_Code: 94025 
              Country: USA 
      Process_Step: 
        Process_Description: Dataset moved. 
        Source_Used_Citation_Abbreviation: 
        d:\workspace\coverages\final_open_file\faults 
      Process_Step: 
        Process_Description: Metadata imported. 
        Source_Used_Citation_Abbreviation: 
        C:\DOCUME~1\ADMINI~1\LOCALS~1\Temp\xml8.tmp 



  Spatial_Data_Organization_Information: 
    Direct_Spatial_Reference_Method: Vector 
    Point_and_Vector_Object_Information: 
      SDTS_Terms_Description: 
        SDTS_Point_and_Vector_Object_Type: Complete chain 
        Point_and_Vector_Object_Count: 1126 
      SDTS_Terms_Description: 
        SDTS_Point_and_Vector_Object_Type: Point 
        Point_and_Vector_Object_Count: 4 
      SDTS_Terms_Description: 
        SDTS_Point_and_Vector_Object_Type: Label point 
        Point_and_Vector_Object_Count: 0 



  Spatial_Reference_Information: 
    Horizontal_Coordinate_System_Definition: 
      Planar: 
        Map_Projection: 
          Map_Projection_Name: Albers Conical Equal Area 
          Albers_Conical_Equal_Area: 
            Standard_Parallel: 55.000000 
            Standard_Parallel: 65.000000 
            Longitude_of_Central_Meridian: -154.000000 
            Latitude_of_Projection_Origin: 50.000000 
            False_Easting: 0.000000 
            False_Northing: 0.000000 
        Planar_Coordinate_Information: 
          Planar_Coordinate_Encoding_Method: coordinate pair 
          Coordinate_Representation: 
            Abscissa_Resolution: 0.008192 
            Ordinate_Resolution: 0.008192 
          Planar_Distance_Units: meters 
      Geodetic_Model: 
        Horizontal_Datum_Name: D_Clarke_1866 
        Ellipsoid_Name: Clarke 1866 
        Semi-major_Axis: 6378206.400000 
        Denominator_of_Flattening_Ratio: 294.978698 



  Entity_and_Attribute_Information: 
    Detailed_Description: 
      Entity_Type: 
        Entity_Type_Label: faults.aat 
      Attribute: 
        Attribute_Label: FID 
        Attribute_Definition: Internal feature number. 
        Attribute_Definition_Source: ESRI 
        Attribute_Domain_Values: 
          Unrepresentable_Domain: 
          Sequential unique whole numbers that are automatically generated. 
      Attribute: 
        Attribute_Label: Shape 
        Attribute_Definition: Feature geometry. 
        Attribute_Definition_Source: ESRI 
        Attribute_Domain_Values: 
          Unrepresentable_Domain: Coordinates defining the features. 
      Attribute: 
        Attribute_Label: FNODE# 
        Attribute_Definition: Internal node number for the beginning of an arc 
        (from-node). 
        Attribute_Definition_Source: ESRI 
        Attribute_Domain_Values: 
          Unrepresentable_Domain: Whole numbers that are automatically 
          generated. 
      Attribute: 
        Attribute_Label: TNODE# 
        Attribute_Definition: Internal node number for the end of an arc 
        (to-node). 
        Attribute_Definition_Source: ESRI 
        Attribute_Domain_Values: 
          Unrepresentable_Domain: Whole numbers that are automatically 
          generated. 
      Attribute: 
        Attribute_Label: LPOLY# 
        Attribute_Definition: Internal node number for the left polygon. 
        Attribute_Definition_Source: ESRI 
        Attribute_Domain_Values: 
          Unrepresentable_Domain: Whole numbers that are automatically 
          generated. 
      Attribute: 
        Attribute_Label: RPOLY# 
        Attribute_Definition: Internal node number for the right polygon. 
        Attribute_Definition_Source: ESRI 
        Attribute_Domain_Values: 
          Unrepresentable_Domain: Whole numbers that are automatically 
          generated. 
      Attribute: 
        Attribute_Label: LENGTH 
        Attribute_Definition: Length of feature in internal units. 
        Attribute_Definition_Source: ESRI 
        Attribute_Domain_Values: 
          Unrepresentable_Domain: Positive real numbers that are automatically 
          generated. 
      Attribute: 
        Attribute_Label: FAULTS# 
        Attribute_Definition: Internal feature number. 
        Attribute_Definition_Source: ESRI 
        Attribute_Domain_Values: 
          Unrepresentable_Domain: 
          Sequential unique whole numbers that are automatically generated. 
      Attribute: 
        Attribute_Label: FAULTS-ID 
        Attribute_Definition: User-defined feature number. 
        Attribute_Definition_Source: ESRI 
      Attribute: 
        Attribute_Label: LTYPE 
        Attribute_Definition: Type of fault, fold axis, or other structural 
        linear feature. 
        Attribute_Definition_Source: author 
        Attribute_Domain_Values: 
          Enumerated_Domain: 
            Enumerated_Domain_Value: anticline 
            Enumerated_Domain_Value_Definition: Surface trace of the axis of an 
            anticline. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: anticlinorium 
            Enumerated_Domain_Value_Definition: 
            The surface trace of the axis of a very large anticline of regional 
            extent 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: anticlinorium inferred 
            Enumerated_Domain_Value_Definition: 
            The surface trace of the axis of a very large anticline of regional 
            extent whose location has not been directly observed. The existence 
            of the fold is inferred from structural and stratigraphic 
            relationships observed elsewhere. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: fault 
            Enumerated_Domain_Value_Definition: 
            Structural boundary between mapped units or structural discontinuity 
            within a mapped unit that has experienced relative offset between 
            the rock bodies on either side of the boundary. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: fault - inferred 
            Enumerated_Domain_Value_Definition: 
            Structural boundary between mapped units or structural discontinuity 
            within a mapped unit that has experienced relative offset between 
            the rock bodies on either side of the boundary. The fault has not 
            been observed, but its existence is inferred from structural and 
            stratigraphic relationships observed elsewhere. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: fold 
            Enumerated_Domain_Value_Definition: Surface trace of the axis of a 
            fold of unspecified orientation. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: gravity high 
            Enumerated_Domain_Value_Definition: location of an observed Bouguer 
            gravity high 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: gravity low 
            Enumerated_Domain_Value_Definition: location of an observed Bouguer 
            gravity low 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: normal 
            Enumerated_Domain_Value_Definition: 
            Surface location of a fault in which the hanging wall has moved 
            downward relative to the footwall. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: normal inferred 
            Enumerated_Domain_Value_Definition: 
            Surface location of a fault in which the hanging wall has moved 
            downward relative to the footwall. The fault has not been observed, 
            but its existence is inferred from structural and stratigraphic 
            relationships observed elsewhere. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: strike slip right 
            Enumerated_Domain_Value_Definition: 
            Location of a fault along which the slip motion is to the right, and 
            parallel to the strike of the fault 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: strike slip right inferred 
            Enumerated_Domain_Value_Definition: 
            Location of a fault along which the slip motion is to the right, and 
            parallel to the strike of the fault. The fault has not been 
            observed, but its existence is inferred from structural and 
            stratigraphic relationships observed elsewhere. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: syncline 
            Enumerated_Domain_Value_Definition: The surface trace of the axis of 
            a syncline 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: synclinorium 
            Enumerated_Domain_Value_Definition: 
            The surface trace of the axis of a very large syncline of regional 
            extent. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: synclinorium inferred 
            Enumerated_Domain_Value_Definition: 
            The surface trace of the axis of a very large syncline of regional 
            extent whose location has not been directly observed. The existence 
            of the fold is inferred from structural and stratigraphic 
            relationships observed elsewhere. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: thrust 
            Enumerated_Domain_Value_Definition: 
            Location of fault in which the dip of the fault is less than 45 
            degrees over much if not all of its length and is characterized by 
            horizontal compression. 
            Enumerated_Domain_Value_Definition_Source: author 
          Enumerated_Domain: 
            Enumerated_Domain_Value: thrust inferred 
            Enumerated_Domain_Value_Definition: 
            Location of fault in which the dip of the fault is less than 45 
            degrees over much if not all of its length and is characterized by 
            horizontal compression. The fault has not been observed, but its 
            existence is inferred from structural and stratigraphic 
            relationships observed elsewhere. 
            Enumerated_Domain_Value_Definition_Source: author 



  Distribution_Information: 
    Distributor: 
      Contact_Information: 
        Contact_Organization_Primary: 
          Contact_Organization: US Geological Survey 
        Contact_Address: 
          Address_Type: mailing address 
          Address: 345 Middlefield Road 
          City: Menlo Park 
          State_or_Province: CA 
          Postal_Code: 94025 
          Country: USA 
    Resource_Description: 
    Downloadable COVERAGE (ARCInfo vector data) format. Coverages are stored in 
    uncompressed ARC export format (ARCInfo version 8.1.2). ArcInfo export files 
    (files with the .e00 file extension) can be converted into ARCInfo coverages 
    in ARCInfo and can be read by some other Geographic Information Systems, 
    such as MapInfo via ARCLink and ESRI's ArcView (limited versions of this 
    software are available for free from ESRI's web site: 
    <http://www.esri.com>). 
    Distribution_Liability: 
    The U.S. Geological Survey (USGS) provides these geographic data "as is." 
    The USGS makes no guarantee or warranty concerning the accuracy of 
    information contained in the geographic data. The USGS further makes no 
    warranties, either expressed or implied, as to any other matter whatsoever, 
    including, without limitation, the condition of the product, or its fitness 
    for any particular purpose. The burden for determining fitness for use lies 
    entirely with the user. Although these data have been processed successfully 
    on computers at the USGS, no warranty, expressed or implied, is made by the 
    USGS regarding the use of these data on any other system, nor does the fact 
    of distribution constitute or imply any such warranty. In no event shall the 
    USGS have any liability whatsoever for payment of any consequential, 
    incidental, indirect, special, or tort damages of any kind, including, but 
    not limited to, any loss of profits arising out of use of or reliance on the 
    geographic data or arising out of the delivery, installation, operation, or 
    support by USGS. This digital database of historic indication of petroleum 
    in the central Alaska province is 1:2,500,000 map-scale and any derivative 
    maps thereof, is not meant to be used or displayed at any scale larger than 
    1:2,500,000. 
    Standard_Order_Process: 
      Digital_Form: 
        Digital_Transfer_Information: 
          Transfer_Size: 0.254 



  Metadata_Reference_Information: 
    Metadata_Date: 20030106 
    Metadata_Review_Date: 2002 
    Metadata_Future_Review_Date: none 
    Metadata_Contact: 
      Contact_Information: 
        Contact_Person_Primary: 
          Contact_Person: Sandra Troutman 
          Contact_Organization: US Geological Survey 
        Contact_Organization_Primary: 
          Contact_Organization: 
          REQUIRED: The organization responsible for the metadata information. 
          Contact_Person: REQUIRED: The person responsible for the metadata 
          information. 
        Contact_Position: GIS Specialist 
        Contact_Address: 
          Address_Type: mailing address 
          Address: 345 Middlefield Road MS 969 
          City: Menlo Park 
          State_or_Province: California 
          Postal_Code: 94025 
          Country: USA 
        Contact_Voice_Telephone: 650-329-4974 
        Contact_Facsimile_Telephone: 650-329-4975 
        Contact_Electronic_Mail_Address: stroutman@usgs.gov 
        Hours_of_Service: Business Hours PST 
    Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial 
    Metadata 
    Metadata_Standard_Version: FGDC-STD-001-1998 
    Metadata_Time_Convention: local time 
    Metadata_Access_Constraints: none 
    Metadata_Use_Constraints: none 
    Metadata_Security_Information: 
      Metadata_Security_Classification_System: none 
      Metadata_Security_Classification: Unclassified 
    Metadata_Extensions: 
      Online_Linkage: <http://www.esri.com/metadata/esriprof80.html> 
      Profile_Name: ESRI Metadata Profile 


Generated by mp version 2.7.3 on Mon Jan 06 15:56:49 2003

