Rowid_,L_TAG,L_DEF,L_EXP
,CL1,.CLNB.,.cartographic line.map boundary.
,CL2,.CLNW.,.cartographic line.water boundary.
,C1,.CONG.DIS.IDC.OBS.MEE.,.generic contact.discrete.identity certain.observable.location meets map accuracy standard.
,C2,.CONG.DIS.IDC.OBS.MNM.,.generic contact.discrete.identity certain.observable.location may not meet map accuracy standard.
,C3,.CONG.DIS.IDC.INF.MNM.,.generic contact.discrete.identity certain.inferred.location may not meet map accuracy standard.
,C4,.CONG.DIS.IDC.INFM.MNM.,.generic contact.discrete.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C5,.CONG.DIS.IDC.INFU.MNM.,.generic contact.discrete.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C6,.CONG.DIS.IDQ.INF.MNM.,.generic contact.discrete.identity questionable.inferred.location may not meet map accuracy standard.
,C7,.CONG.DIS.IDQ.INFM.MNM., .generic contact.discrete.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C8,.CONG.DIS.INFU.MNM.,.generic contact.discrete.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C9,.CONG.GRD.IDC.OBS.MEE.,.generic contact.gradational.identity certain.observable.location meets map accuracy standard.
,C10,.CONG.GRD.IDC.OBS.MNM.,.generic contact.gradational.identity certain.observable.location may not meet map accuracy standard.
,C11,.CONG.GRD.IDC.INF.MNM.,.generic contact.gradational.identity certain.inferred.location may not meet map accuracy standard.
,C12,.CONG.GRD.IDC.INFM.MNM.,.generic contact.gradational.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C13,.CONG.GRD.IDC.INFU.MNM.,.generic contact.gradational.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C14,.CONG.GRD.IDQ.INF.MNM.,.generic contact.gradational.identity questionable.inferred.location may not meet map accuracy standard.
,C15,.CONG.GRD.IDQ.INFM.MNM.,.generic contact.gradational.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C16,.CONG.GRD.IDQ.INFU.MNM.,.generic contact.gradational.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C17,.CONL.DIS.IDC.OBS.MEE.,.landslide contact.discrete.identity certain.observable.location meets map accuracy standard.
,C18,.CONL.DIS.IDC.OBS.MNM.,.landslide contact.discrete.identity certain.observable.location may not meet map accuracy standard.
,C19,.CONL.DIS.IDC.INF.MNM.,.landslide contact.discrete.identity certain.inferred.location may not meet map accuracy standard.
,C20,.CONL.DIS.IDC.INFM.MNM.,.landslide contact.discrete.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C21,.CONL.DIS.IDC.INFU.MNM.,.landslide contact.discrete.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C22,.CONL.DIS.IDQ.INF.MNM.,.landslide contact.discrete.identity questionable.inferred.location may not meet map accuracy standard.
,C23,.CONL.DIS.IDQ.INFM.MNM.,.landslide contact.discrete.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C24,.CONL.DIS.INFU.MNM.,.landslide contact.discrete.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C25,.CONL.CRW.IDC.OBS.MEE.,.landslide contact.crown scarp.identity certain.observable.location meets map accuracy standard.
,C26,.CONL.CRW.IDC.OBS.MNM.,.landslide contact.crown scarp.identity certain.observable.location may not meet map accuracy standard.
,C27,.CONL.CRW.IDC.INF.MNM.,.landslide contact.crown scarp.identity certain.inferred.location may not meet map accuracy standard.
,C28N,.CONL.CRW.IDQ.MNM.,.landslide contact.crown scarp.identity questionable.inferred.location may not meet map accuracy standard.
,C29,.CONS.DIS.IDC.OBS.MEE.,.sedimentary contact.discrete.identity certain.observable.location meets map accuracy standard.
,C30,.CONS.DIS.IDC.OBS.MNM.,.sedimentary contact.discrete.identity certain.observable.location may not meet map accuracy standard.
,C31,.CONS.DIS.IDC.INF.MNM.,.sedimentary contact.discrete.identity certain.inferred.location may not meet map accuracy standard.
,C32,.CONS.DIS.IDC.INFM.MNM.,.sedimentary contact.discrete.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C33,.CONS.DIS.IDC.INFU.MNM.,.sedimentary contact.discrete.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C34,.CONS.DIS.IDQ.INF.MNM.,.sedimentary contact.discrete.identity questionable.inferred.location may not meet map accuracy standard.
,C35,.CONS.DIS.IDQ.INFM.MNM.,.sedimentary contact.discrete.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C36,.CONS.DIS.INFU.MNM.,.sedimentary contact.discrete.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C37,.CONST.DIS.IDC.OBS.MEE.,.sedimentary contact.discrete.separates terraced alluvial units.identity certain.observable.location meets map accuracy standard.
,C38,.CONS.CONST.IDC.OBS.MNM.,.sedimentary contact.discrete.separates terraced alluvial units.identity certain.observable.location may not meet map accuracy standard.
,C39,.CONS.CONST.IDC.INF.MNM.,.sedimentary contact.discrete.separates terraced alluvial units.identity certain.inferred.location may not meet map accuracy standard.
,C40N,.CONS.CONST.IDQ.INF.MNM.,.sedimentary contact.discrete.separates terraced alluvial units.identity questionable.inferred.location may not meet map accuracy standard.
,C41,.CONS.GRD.IDC.OBS.MEE.,.sedimentary contact.gradational.identity certain.observable.location meets map accuracy standard.
,C42,.CONS.GRD.IDC.OBS.MNM.,.sedimentary contact.gradational.identity certain.observable.location may not meet map accuracy standard.
,C43,.CONS.GRD.IDC.INF.MNM.,.sedimentary contact.gradational.identity certain.inferred.location may not meet map accuracy standard.
,C44,.CONS.GRD.IDC.INFM.MNM.,.sedimentary contact.gradational.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C45,.CONS.GRD.IDC.INFU.MNM.,.sedimentary contact.gradational.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C46,.CONS.GRD.IDQ.INF.MNM.,.sedimentary contact.gradational.identity questionable.inferred.location may not meet map accuracy standard.
,C47,.CONS.GRD.IDQ.INFM.MNM.,.sedimentary contact.gradational.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C48,.CONS.GRD.IDQ.INFU.MNM.,.sedimentary contact.gradational.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C49,.CONI.DIS.IDC.OBS.MEE.,.igneous contact.discrete.identity certain.observable.location meets map accuracy standard.
,C50,.CONI.DIS.IDC.OBS.MNM.,.igneous contact.discrete.identity certain.observable.location may not meet map accuracy standard.
,C51,.CONI.DIS.IDC.INF.MNM.,.igneous contact.discrete.identity certain.inferred.location may not meet map accuracy standard.
,C52,.CONI.DIS.IDC.INFM.MNM.,.igneous contact.discrete.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C53,.CONI.DIS.IDC.INFU.MNM.,.igneous contact.discrete.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C54,.CONI.DIS.IDQ.INF.MNM.,.igneous contact.discrete.identity questionable.inferred.location may not meet map accuracy standard.
,C55,.CONI.DIS.IDQ.INFM.MNM.,.igneous contact.discrete.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C56,.CONI.DIS.INFU.MNM.,.igneous contact.discrete.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C57,.CONI.GRD.IDC.OBS.MEE.,.igneous contact.gradational.identity certain.observable.location meets map accuracy standard.
,C58,.CONI.GRD.IDC.OBS.MNM.,.igneous contact.gradational.identity certain.observable.location may not meet map accuracy standard.
,C59,.CONI.GRD.IDC.INF.MNM.,.igneous contact.gradational.identity certain.inferred.location may not meet map accuracy standard.
,C60,.CONI.GRD.IDC.INFM.MNM.,.igneous contact.gradational.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C61,.CONI.GRD.IDC.INFU.MNM.,.igneous contact.gradational.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C62,.CONI.GRD.IDQ.INF.MNM.,.igneous contact.gradational.identity questionable.inferred.location may not meet map accuracy standard.
,C63,.CONI.GRD.IDQ.INFM.MNM.,.igneous contact.gradational.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C64,.CONI.GRD.IDQ.INFU.MNM.,.igneous contact.gradational.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C65,.CONM.DIS.IDC.OBS.MEE.,.metamorphic contact.discrete.identity certain.observable.location meets map accuracy standard.
,C66,.CONM.DIS.IDC.OBS.MNM.,.metamorphic contact.discrete.identity certain.observable.location may not meet map accuracy standard.
,C67,.CONM.DIS.IDC.INF.MNM.,.metamorphic contact.discrete.identity certain.inferred.location may not meet map accuracy standard.
,C68,.CONM.DIS.IDC.INFM.MNM.,.metamorphic contact.discrete.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C69,.CONM.DIS.IDC.INFU.MNM.,.metamorphic contact.discrete.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C70,.CONM.DIS.IDQ.INF.MNM.,.metamorphic contact.discrete.identity questionable.inferred.location may not meet map accuracy standard.
,C71,.CONM.DIS.IDQ.INFM.MNM.,.metamorphic contact.discrete.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C72,.CONM.DIS.INFU.MNM.,.metamorphic contact.discrete.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C73,.CONM.GRD.IDC.OBS.MEE.,.metamorphic contact.gradational.identity certain.observable.location meets map accuracy standard.
,C74,.CONM.GRD.IDC.OBS.MNM.,.metamorphic contact.gradational.identity certain.observable.location may not meet map accuracy standard.
,C75,.CONM.GRD.IDC.INF.MNM.,.metamorphic contact.gradational.identity certain.inferred.location may not meet map accuracy standard.
,C76,.CONM.GRD.IDC.INFM.MNM.,.metamorphic contact.gradational.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C77,.CONM.GRD.IDC.INFU.MNM.,.metamorphic contact.gradational.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C78,.CONM.GRD.IDQ.INF.MNM.,.metamorphic contact.gradational.identity questionable.inferred.location may not meet map accuracy standard.
,C79,.CONM.GRD.IDQ.INFM.MNM.,.metamorphic contact.gradational.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C80,.CONM.GRD.IDQ.INFU.MNM.,.metamorphic contact.gradational.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C81,.CONR.DIS.IDC.OBS.MEE.,.regolith or pedogenic soil contact.discrete.identity certain.observable.location meets map accuracy standard.
,C82,.CONR.DIS.IDC.OBS.MNM.,.regolith or pedogenic soil contact.discrete.identity certain.observable.location may not meet map accuracy standard.
,C83,.CONR.DIS.IDC.INF.MNM.,.regolith or pedogenic soil contact.discrete.identity certain.inferred.location may not meet map accuracy standard.
,C84,.CONR.DIS.IDC.INFM.MNM.,.regolith or pedogenic soil contact.discrete.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C85,.CONR.DIS.IDC.INFU.MNM.,.regolith or pedogenic soil contact.discrete.identity certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C86,.CONR.DIS.IDQ.INF.MNM.,.regolith or pedogenic soil contact.discrete.identity questionable.inferred.location may not meet map accuracy standard.
,C87,.CONR.DIS.IDQ.INFM.MNM.,.regolith or pedogenic soil contact.discrete.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,C88,.CONR.DIS.INFU.MNM.,.regolith or pedogenic soil contact.discrete.identity questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,C89,.COND.GPH.GPHA.MNM.,.contact inferred by indirect methods.geophysics.aeromagnetic survey.location may not meet map accuracy standard.
,C90,.COND.GPH.GPHM.MNM.,.contact inferred by indirect methods.geophysics.ground magnetic survey.location may not meet map accuracy standard.
,C91,.COND.GPH.GPHG.MNM.,.contact inferred by indirect methods.geophysics.gravity survey.location may not meet map accuracy standard.
,C92,.COND.GPH.GPHR.MNM.,.contact inferred by indirect methods.geophysics.radiometric survey.location may not meet map accuracy standard.
,C93,.COND.RSI.MNM.,.contact inferred by indirect methods.remote sensing imagery.location may not meet map accuracy standard.
,C94,.COND.GWL.MNM.,.contact inferred by indirect methods.ground water levels.location may not meet map accuracy standard.
,C95,.COND.SSB.MNM.,.contact inferred by indirect methods.subsurface boring data.location may not meet map accuracy standard.
,C96,.CONKG.,.contact
,C97,.CONKL.,.contact
,C98,.CONKS.,.contact
,C99,.CONKI.,.contact
,C100,.CONKM.,.contact
,C101,.CONKR.,.contact
,MH1,.MMHB.IDC.OBS.LOW.,.mapped marker horizon.buried paleosol.identity certain.observable.located well but may not meet map accuracy standard.
,MH2,.MMHB.IDC.INFM.MNM.,.mapped marker horizon.buried paleosol.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,MH3,.MMHV.IDC.OBS.LOW.,.mapped marker horizon.volcanic flow.identity certain.observable.located well but may not meet map accuracy standard.
,MH4,.MMHV.IDC.INFM.MNM.,.mapped marker horizon.volcanic flow.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,MH5,.MMHA.IDC.OBS.LOW.,.mapped marker horizon.volcanic ash layer.identity certain.observable.located well but may not meet map accuracy standard.
,MH6,.MMHA.IDC.INFM.MNM.,.mapped marker horizon.volcanic ash layer.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,MH7,.MMHG.IDC.OBS.LOW.,.mapped marker horizon.gravel layer.identity certain.observable.located well but may not meet map accuracy standard.
,MH8,.MMHG.IDC.INFM.MNM.,.mapped marker horizon.gravel layer.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,MH9,.MMH.IDC.OBS.LOW.,.mapped marker horizon.identity certain.observable.located well but may not meet map accuracy standard.
,MH10,.MMH.IDC.INFM.MNM.,.mapped marker horizon.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,MH11,.MMH.IDC.OBS.LOW.,.mapped marker horizon.identity certain.observable.located well but may not meet map accuracy standard.
,MH12,.MMH.IDC.INFM.MNM.,.mapped marker horizon.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F1,.FLTH.SLPUG.EXC.OBS.MEE.,.high-angle fault.slip unspecified.generic fault.existence certain.observable.location meets map accuracy standard.
,F2,.FLTH.SLPSR.EXC.OBS.MEE.,.high-angle fault.strike slip.right lateral fault.existence certain.observable.location meets map accuracy standard.
,F3,.FLTH.SLPSL.EXC.OBS.MEE.,.high-angle fault.strike slip.left lateral fault.existence certain.observable.location meets map accuracy standard.
,F4,.FLTH.SLPNN.EXC.OBS.MEE.,.high-angle fault.normal slip.normal fault.existence certain.observable.location meets map accuracy standard.
,F5,.FLTH.SLPRR.EXC.OBS.MEE.,.high-angle fault.reverse slip.reverse fault.existence certain.observable.location meets map accuracy standard.
,F6,.FLTH.SLPOO.EXC.OBS.MEE.,.high-angle fault.oblique slip.oblique fault.existence certain.observable.location meets map accuracy standard.
,F7,.FLTH.SLPUG.EXC.OBS.MNM.,.high-angle fault.slip unspecified.generic fault.existence certain.observable.location may not meet map accuracy standard.
,F8,.FLTH.SLPSR.EXC.OBS.MNM.,.high-angle fault.strike slip.right lateral fault.existence certain.observable.location may not meet map accuracy standard.
,F9,.FLTH.SLPSL.EXC.OBS.MNM.,.high-angle fault.strike slip.left lateral fault.existence certain.observable.location may not meet map accuracy standard.
,F10,.FLTH.SLPNN.EXC.OBS.MNM.,.high-angle fault.normal slip.normal fault.existence certain.observable.location may not meet map accuracy standard.
,F11,.FLTH.SLPRR.EXC.OBS.MNM.,.high-angle fault.reverse slip.reverse fault.existence certain.observable.location may not meet map accuracy standard.
,F12,.FLTH.SLPOO.EXC.OBS.MNM.,.high-angle fault.oblique slip.oblique fault.existence certain.observable.location may not meet map accuracy standard.
,F13,.FLTH.SLPUG.EXC.INF.MNM.,.high-angle fault.slip unspecified.generic fault.existence certain.inferred.location may not meet map accuracy standard.
,F14,.FLTH.SLPSR.EXC.INF.MNM.,.high-angle fault.strike slip.right lateral fault.existence certain.inferred.location may not meet map accuracy standard.
,F15,.FLTH.SLPSL.EXC.INF.MNM.,.high-angle fault.strike slip.left lateral fault.existence certain.inferred.location may not meet map accuracy standard.
,F16,.FLTH.SLPNN.EXC.INF.MNM.,.high-angle fault.normal slip.normal fault.existence certain.inferred.location may not meet map accuracy standard.
,F17,.FLTH.SLPRR.EXC.INF.MNM.,.high-angle fault.reverse slip.reverse fault.existence certain.inferred.location may not meet map accuracy standard.
,F18,.FLTH.SLPOO.EXC.INF.MNM.,.high-angle fault.oblique slip.oblique fault.existence certain.inferred.location may not meet map accuracy standard.
,F19,.FLTH.SLPUG.EXC.INFM.MNM.,.high-angle fault.slip unspecified.generic fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F20,.FLTH.SLPSR.EXC.INFM.MNM.,.high-angle fault.strike slip.right lateral fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F21,.FLTH.SLPSL.EXC.INFM.MNM.,.high-angle fault.strike slip.left lateral fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F22,.FLTH.SLPNN.EXC.INFM.MNM.,.high-angle fault.normal slip.normal fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F23,.FLTH.SLPR.SLPRR.EXC.INFM.MNM.,.high-angle fault.reverse slip.reverse fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F24,.FLTH.SLPO.SLPOO.EXC.INFM.MNM.,.high-angle fault.oblique slip.oblique fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F25,.FLTH.SLPUG.EXC.INFU.MNM.,.high-angle fault.slip unspecified.generic fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F26,.FLTH.SLPSR.EXC.INFU.MNM.,.high-angle fault.strike slip.right lateral fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F27,.FLTH.SLPSL.EXC.INFU.MNM.,.high-angle fault.strike slip.left lateral fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F28,.FLTH.SLPNN.EXC.INFU.MNM.,.high-angle fault.normal slip.normal fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F29,.FLTH.SLPRR.EXC.INFU.MNM.,.high-angle fault.reverse slip.reverse fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F30,.FLTH.SLPOO.EXC.INFU.MNM.,.high-angle fault.oblique slip.oblique fault.existence certain.inferred beneath unmapped covering unit. location may not meet map accuracy standard.
,F31,.FLTH.SLPUG.EXQ.INF.MNM.,.high-angle fault.slip unspecified.generic fault.existence questionable.inferred.location may not meet map accuracy standard.
,F32,.FLTH.SLPSR.EXQ.INF.MNM.,.high-angle fault.strike slip.right lateral fault.existence questionable.inferred.location may not meet map accuracy standard.
,F33,.FLTH.SLPSL.EXQ.INF.MNM.,.high-angle fault.strike slip.left lateral fault.existence questionable.inferred.location may not meet map accuracy standard.
,F34,.FLTH.SLPNN.EXQ.INF.MNM.,.high-angle fault.normal slip.normal fault.existence questionable.inferred.location may not meet map accuracy standard.
,F35,.FLTH.SLPRR.EXQ.INF.MNM.,.high-angle fault.reverse slip.reverse fault.existence questionable.inferred.location may not meet map accuracy standard.
,F36,.FLTH.SLPOO.EXQ.INF.MNM.,.high-angle fault.oblique slip.oblique fault.existence questionable.inferred.location may not meet map accuracy standard.
,F37,.FLTH.SLPUG.EXQ.INFM.MNM.,.high-angle fault.slip unspecified.generic fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F38,.FLTH.SLPSR.EXQ.INFM.MNM.,.high-angle fault.strike slip.right lateral fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F39,.FLTH.SLPSL.EXQ.INFM.MNM.,.high-angle fault.strike slip.left lateral fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F40,.FLTH.SLPNN.EXQ.INFM.MNM.,.high-angle fault.normal slip.normal fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F41,.FLTH.SLPRR.EXQ.INFM.MNM.,.high-angle fault.reverse slip.reverse fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F42,.FLTH.SLPOO.EXQ.INFM.MNM.,.high-angle fault.oblique slip.oblique fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F43,.FLTH.SLPUG.EXQ.INFU.MNM.,.high-angle fault.slip unspecified.generic fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F44,.FLTH.SLPSR.EXQ.INFU.MNM.,.high-angle fault.strike slip.right lateral fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F45,.FLTH.SLPSL.EXQ.INFU.MNM.,.high-angle fault.strike slip.left lateral fault.existence questionable.inferred beneath unmapped covering unit.may not meet map accuracy standard.
,F46,.FLTH.SLPNN.EXQ.INFU.MNM.,.high-angle fault.normal slip.normal fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F47,.FLTH.SLPRR.EXQ.INFU.MNM.,.high-angle fault.reverse slip.reverse fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F48,.FLTH.SLPOO.EXQ.INFU.MNM.,.high-angle fault.oblique slip.oblique fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F49,.FLTH.SLPUG.FSC.IDC.MEE.,.high-angle fault.slip unspecified.generic fault.scarp.identity certain.location meets map accuracy standard.
,F50,.FLTH.SLPSR.FSC.IDC.MEE.,.high-angle fault.strike slip.right lateral fault.scarp.identity certain.location meets map accuracy standard.
,F51,.FLTH.SLPSL.FSC.IDC.MEE.,.high-angle fault.strike slip.left lateral fault.scarp.identity certain.location meets map accuracy standard.
,F52,.FLTH.SLPNN.FSC.IDC.MEE.,.high-angle fault.normal slip.normal fault.scarp.identity certain.location meets map accuracy standard.
,F53,.FLTH.SLPRR.FSC.IDC.MEE.,.high-angle fault.reverse slip.reverse fault.scarp.identity certain.location meets map accuracy standard.
,F54,.FLTH.SLPOO.FSC.IDC.MEE.,.high-angle fault.oblique slip.oblique fault.scarp.identity certain.location meets map accuracy standard.
,F55,.FLTH.SLPUG.FSC.IDC.MNM.,.high-angle fault.slip unspecified.generic fault.scarp.identity certain.location may not meet map accuracy standard.
,F56,.FLTH.SLPSR.FSC.IDC.MNM.,.high-angle fault.strike slip.right lateral fault.scarp.identity certain.location may not meet map accuracy standard.
,F57,.FLTH.SLPSL.FSC.IDC.MNM.,.high-angle fault.strike slip.left lateral fault.scarp.identity certain.location may not meet map accuracy standard.
,F58,.FLTH.SLPNN.FSC.IDC.MNM.,.high-angle fault.normal slip.normal fault.scarp.identity certain.location may not meet map accuracy standard.
,F59,.FLTH.SLPRR.FSC.IDC.MNM.,.high-angle fault.reverse slip.reverse fault.scarp.identity certain.location may not meet map accuracy standard.
,F60,.FLTH.SLPOO.FSC.IDC.MNM.,.high-angle fault.oblique slip.oblique fault.scarp.identity certain.location may not meet map accuracy standard.
,F61N,.FLTH.SLPUG.FSC.IDQ.PRO.MNM.,.high-angle fault.slip unspecified.generic fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F62N,.FLTH.SLPUG.FSC.IDQ.POS.MNM.,.high-angle fault.slip unspecified.generic fault.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F63N,.FLTH.SLPSR.FSC.IDQ.PRO.MNM.,.high-angle fault.strike slip.right lateral fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F64N,.FLTH.SLPSR.FSC.IDQ.POS.MNM.,.high-angle fault.strike slip.right lateral fault.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F65N,.FLTH.SLPSL.FSC.IDQ.PRO.MNM.,.high-angle fault.strike slip.left lateral fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F66N,.FLTH.SLPSL.FSC.IDQ.POS.MNM.,.high-angle fault.strike slip.left lateral fault.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F67N,.FLTH.SLPNN.FSC.IDQ.PRO.MNM.,.high-angle fault.normal slip.normal fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F68N,.FLTH.SLPNN.FSC.IDQ.POS.MNM.,.high-angle fault.normal slip.normal fault.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F69N,.FLTH.SLPRR.FSC.IDQ.PRO.MNM.,.high-angle fault.reverse slip.reverse fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F70N,.FLTH.SLPRR.FSC.IDQ.POS.MNM.,.high-angle fault.reverse slip.reverse fault.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F71N,.FLTH.SLPOO.FSC.IDQ.PRO.MNM.,.high-angle fault.oblique slip.oblique fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F72N,.FLTH.SLPOO.FSC.IDQ.POS.MNM.,.high-angle fault.oblique slip.oblique fault.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F73,.FLTL.SLPUL.WRLU.EXC.OBS.MEE.,.fault.low angle.slip unspecified.fault wall relations unspecified.low angle fault.existence certain.observable.location meets map accuracy standard.
,F74,.FLTL.SLPUL.WRLU.EXC.OBS.MNM.,.fault.low angle.slip unspecified.fault wall relations unspecified.low angle fault.existence certain.observable.location may not meet map accuracy standard.
,F75,.FLTL.SLPUL.WRLU.EXC.INF.MNM.,.fault.low angle.slip unspecified.fault wall relations unspecified.low angle fault.existence certain.inferred.location may not meet map accuracy standard.
,F76,.FLTL.SLPUL.WRLU.EXC.INFM.MNM.,.fault.low angle.slip unspecified.fault wall relations unspecified.low angle fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F77,.FLTL.SLPUL.WRLU.EXC.INFU.MNM.,.fault.low angle.slip unspecified.fault wall relations unspecified.low angle fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F78,.FLTL.SLPUL.WRLU.EXQ.INF.MNM.,.fault.low angle.slip unspecified.fault wall relations unspecified.low angle fault.existence questionable.inferred.location may not meet map accuracy standard.
,F79,.FLTL.SLPUL.WRLU.EXQ.INFM.MNM.,.fault.low angle.slip unspecified.fault wall relations unspecified.low angle fault.existence questionable.Inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F80,.FLTL.SLPUL.WRLU.EXQ.INFU.MNM.,.fault.low angle.slip unspecified.fault wall relations unspecified.low angle fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F81,.FLTL.SLPUL.WRLY.EXC.OBS.MEE.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence certain.observable.location meets map accuracy standard.
,F82,.FLTL.SLPUL.WRLY.EXC.OBS.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence certain.observable.location may not meet map accuracy standard.
,F83,.FLTL.SLPUL.WRLY.EXC.INF.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence certain.inferred.location may not meet map accuracy standard.
,F84,.FLTL.SLPUL.WRLY.EXC.INFM.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F85,.FLTL.SLPUL.WRLY.EXC.INFU.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F86N,.FLTL.SLPUL.WRLY.EXQ.INF.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence questionable.inferred.location may not meet map accuracy standard.
,F87N,.FLTL.SLPUL.WRLY.EXQ.INFM.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F88N,.FLTL.SLPUL.WRLY.EXQ.INFU.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F89,.FLTL.SLPUL.WRLO.EXC.OBS.MEE.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence certain.observable.location meets map accuracy standard.
,F90,.FLTL.SLPUL.WRLO.EXC.OBS.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence certain.observable.location may not meet map accuracy standard.
,F91,.FLTL.SLPUL.WRLO.EXC.INF.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence certain.nferred.location may not meet map accuracy standard.
,F92,.FLTL.SLPUL.WRLO.EXC.INFM.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F93,.FLTL.SLPUL.WRLO.EXC.INFU.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F94N,.FLTL.SLPUL.WRLO.EXQ.INF.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence questionable.inferred.location may not meet map accuracy standard.
,F95N,.FLTL.SLPUL.WRLO.EXQ.INFM.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F96N,.FLTL.SLPUL.WRLO.EXQ.INFU.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F97,.FLTL.SLPNL.WRLY.EXC.OBS.MEE.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence certain.observable.location meets map accuracy standard.
,F98,.FLTL.SLPNL.WRLY.EXC.EC.OBS.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence certain.observable.location may not meet map accuracy standard.
,F99,.FLTL.SLPNL.WRLY.EXC.INF.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence certain.inferred.location may not meet map accuracy standard.
,F100,.FLTL.SLPNL.WRLY.EXC.INFM.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F101,.FLTL.SLPNL.WRLY.EXC.INFU.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F102N,.FLTL.SLPNL.WRLY.EXQ.INF.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence questionable.inferred.location may not meet map accuracy standard.
,F103N,.FLTL.SLPNL.WRLY.EXQ.INFM.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F104N,.FLTL.SLPNL.WRLY.EXQ.INFU.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F105,.FLTL.SLPNDM.WRLY.EXC.OBS.MEE.,.fault.low angle.normal slip.younger over older.master detachment.existence certain.observable.location meets map accuracy standard.
,F106,.FLTL.SLPNDM.WRLY.EXC.OBS.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence certain.observable.location may not meet map accuracy standard.
,F107,.FLTL.SLPNDM.WRLY.EXC.INF.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence certain.inferred.location may not meet map accuracy standard.
,F108,.FLTL.SLPNDM.WRLY.EXC.INFM.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence certain.nferred beneath mapped covering unit.location may not meet map accuracy standard.
,F109,.FLTL.SLPNDM.WRLY.EXC.INFU.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F110N,.FLTL.SLPNDM.WRLY.EXQ.INF.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F111N,.FLTL.SLPNDM.WRLY.EXQ.INFM.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F112N,.FLTL.SLPNDM.WRLY.EXQ.INFU.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F113,.FLTL.SLPND.WRLY.EXC.OBS.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence certain.observable.location meets map accuracy standard.
,F114,.FLTL.SLPND.WRLY.EXC.OBS.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence certain.observable.location may not meet map accuracy standard.
,F115,.FLTL.SLPND.WRLY.EXC.INF.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence certain.inferred.located well but rarely meets map accuracy standard.
,F116,.FLTL.SLPND.WRLY.EXC.INFM.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence certain.inferred beneath mapped covering unit.located well but rarley meets map accuracy standard.
,F117,.FLTL.SLPND.WRLY.EXC.INFU.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F118N,.FLTL.SLPND.WRLY.EXQ.INF.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F119N,.FLTL.SLPND.WRLY.EXQ.INFM.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F120N,.FLTL.SLPND.WRLY.EXQ.INFU.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F121,.FLTL.SLPNL.WRLY.EXC.OBS.MEE.,.fault.low angle.normal slip.younger over older.listric into detachment.existence certain.observable.location meets map accuracy standard.
,F122,.FLTL.SLPNL.WRLY.EXC.OBS.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence certain.observable.location may not meet map accuracy standard.
,F123,.FLTL.SLPNL.WRLY.EXC.INF.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F124,.FLTL.SLPNL.WRLY.EXC.INFM.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F125,.FLTL.SLPNL.WRLY.EXC.INFU.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F126N,.FLTL.SLPNL.WRLY.EXQ.INF.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F127N,.FLTL.SLPNL.WRLY.EXQ.INFM.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F128N,.FLTL.SLPNL.WRLY.EXQ.INFU.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F129,.FLTL.SLPNDM.WRLO.EXC.OBS.MEE.,.fault.low angle.normal slip.older over younger.master detachment.existence certain.observable.location meets map accuracy standard.
,F130,.FLTL.SLPNDM.WRLO.EXC.OBS.MNM.,.fault.low angle.normal slip.older over younger.master detachment.existence certain.observable.location may not meet map accuracy standard.
,F131,.FLTL.SLPNDM.WRLO.EXC.INF.MNM.,.fault.low angle.normal slip.older over younger.master detachment.existence certain.inferred.location may not meet map accuracy standard.
,F132,.FLTL.SLPNDM.WRLO.EXC.INFM.MNM.,.fault.low angle.normal slip.older over younger.master detachment.existence certain.nferred beneath mapped covering unit.location may not meet map accuracy standard.
,F133,.FLTL.SLPNDM.WRLO.EXC.INFU.MNM.,fault.low angle.normal slip.older over younger.master detachment.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F134N,.FLTL.SLPNDM.WRLO.EXQ.INF.MNM.,.fault.low angle.normal slip.older over younger.master detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F135N,.FLTL.SLPNDM.WRLO.EXQ.INFM.MNM.,.fault.low angle.normal slip.older over younger.master detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F136N,.FLTL.SLPNDM.WRLO.EXQ.INFU.MNM.,.fault.low angle.normal slip.older over younger.master detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F137,.FLTL.SLPND.WRLO.EXC.OBS.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence certain.observable.location meets map accuracy standard.
,F138,.FLTL.SLPND.WRLO.EXC.OBS.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence certain.observable.location may not meet map accuracy standard.
,F139,.FLTL.SLPND.WRLO.EXC.INF.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence certain.inferred.located well but rarely meets map accuracy standard.
,F140,.FLTL.SLPND.WRLO.EXC.INFM.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence certain.inferred beneath mapped covering unit.located well but rarley meets map accuracy standard.
,F141,.FLTL.SLPND.WRLO.EXC.INFU.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F142N,.FLTL.SLPND.WRLO.EXQ.INF.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F143N,.FLTL.SLPND.WRLO.EXQ.INFM.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F144N,.FLTL.SLPND.WRLO.EXQ.INFU.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F145,.FLTL.SLPNL.WRLO.EXC.OBS.MEE.,.fault.low angle.normal slip.older over younger.listric into detachment.existence certain.observable.location meets map accuracy standard.
,F146,.FLTL.SLPNL.WRLO.EXC.OBS.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence certain.observable.location may not meet map accuracy standard.
,F147,.FLTL.SLPNL.WRLO.EXC.INF.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F148,.FLTL.SLPNL.WRLO.EXC.INFM.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F149,.FLTL.SLPNL.WRLO.EXC.INFU.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F150N,.FLTL.SLPNL.WRLO.EXQ.INF.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F151N,.FLTL.SLPNL.WRLO.EXQ.INFM.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F152N,.FLTL.SLPNL.WRLO.EXQ.INFU.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F153,.FLTL.SLPTD.WRLY.EXC.OBS.MEE.,.fault.low angle.thrust slip.younger over older.decollement.existence certain.observable.location meets map accuracy standard.
,F154,.FLTL.SLPTD.WRLY.EXC.OBS.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence certain.observable.location may not meet map accuracy standard.
,F155,.FLTL.SLPTD.WRLY.EXC.INF.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence certain.inferred.location may not meet map accuracy standard.
,F156,.FLTL.SLPTD.WRLY.EXC.INFM.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F157,.FLTL.SLPTD.WRLY.EXC.INFU.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F158N,.FLTL.SLPTD.WRLY.EXQ.INF.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence questionable.inferred.location may not meet map accuracy standard.
,F159N,.FLTL.SLPTD.WRLY.EXQ.INFM.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F160N,.FLTL.SLPTD.WRLY.EXQ.INFU.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F161,.FLTL.SLPTT.WRLY.EXC.OBS.MEE.,.fault.low angle.thrust slip.younger over older.thrust.existence certain.observable.location meets map accuracy standard.
,F162,.FLTL.SLPTT.WRLY.EXC.OBS.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence certain.observable.location may not meet map accuracy standard.
,F163,.FLTL.SLPTT.WRLY.EXC.INF.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence certain.inferred.location may not meet map accuracy standard.
,F164,.FLTL.SLPTT.WRLY.EXC.INFM.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F165,.FLTL.SLPTT.WRLY.EXC.INFU.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F166N,.FLTL.SLPTT.WRLY.EXQ.INF.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence questionable.inferred.location may not meet map accuracy standard.
,F167N,.FLTL.SLPTT.WRLY.EXQ.INFM.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F168N,.FLTL.SLPTT.WRLY.EXQ.INFU.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F169,.FLTL.SLPTTO.WRLY.EXC.OBS.MEE.,.fault.low angle.thrust slip. younger over older.thrust.overturned.existence certain.observable.location meets map accuracy standard.
,F170,.FLTL.SLPTTO.WRLY.EXC.OBS.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence certain.observable.location may not meet map accuracy standard.
,F171,.FLTL.SLPTTO.WRLY.EXC.INF.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence certain.inferred.location may not meet map accuracy standard.
,F172,.FLTL.SLPTTO.WRLY.EXC.INFM.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F173,.FLTL.SLPTTO.WRLY.EXC.INFU.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F174N,.FLTL.SLPTTO.WRLY.EXQ.INF.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence questionable.inferred.location may not meet map accuracy standard.
,F175N,.FLTL.SLPTTO.WRLY.EXQ.INFM.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F176N,.FLTL.SLPTTO.WRLY.EXQ.INFU.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F177,.FLTL.SLPTT.WRLO.EXC.OBS.MEE.,.fault.low angle.thrust slip.older over younger.thrust.existence certain.observable.location meets map accuracy standard.
,F178,.FLTL.SLPTT.WRLO.EXC.OBS.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence certain.observable.location may not meet map accuracy standard.
,F179,.FLTL.SLPTT.WRLO.EXC.INF.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence certain.inferred.location may not meet map accuracy standard.
,F180,.FLTL.SLPTT.WRLO.EXC.INFM.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F181,.FLTL.SLPTT.WRLO.EXC.INFU.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F182N,.FLTL.SLPTT.WRLO.EXQ.INF.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence questionable.inferred.location may not meet map accuracy standard.
,F183N,.FLTL.SLPTT.WRLO.EXQ.INFM.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F184N,.FLTL.SLPTT.WRLO.EXQ.INFU.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F185,.FLTL.SLPTTO.WRLO.EXC.OBS.MEE.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence certain.observable.location meets map accuracy standard.
,F186,.FLTL.SLPTTO.WRLO.EXC.OBS.MNM.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence certain.observable.location may not meet map accuracy standard.
,F187,.FLTL.SLPTTO.WRLO.EXC.INF.MNM.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence certain.inferred.location may not meet map accuracy standard.
,F188,.FLTL.SLPTTO.WRLO.IEC.NFM.MNM.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F189N,.FLTL.SLPTTO.WRLO.EXC.INFU.MNM.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F190N,.FLTL.SLPTTO.WRLO.EXQ.INF.MNM.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence questionable.inferred.location may not meet map accuracy standard.
,F191N,.FLTL.SLPTTO.WRLO.EXQ.INFM.MNM.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F192N,.FLTL.SLPTTO.WRLO.EXQ.INFU.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence questionable.overturned.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F193,.FLTL.SLPTT.WRLO.FSC.IDC.MEE.,.fault.low angle.thrust slip.older over younger.thrust.scarp.identity certain.location meets map accuracy standard.
,F194,.FLTL.SLPTT.WRLO.FSC.IDC.MNM.,.fault.low angle.thrust slip.older over younger.thrust.scarp.identity certain.location may not meet map accuracy standard.
,F195N,.FLTL.SLPTT.WRLO.FSC.IDQ.PRO.MNM.,.fault.low angle.thrust slip.older over younger.thrust.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F196N,.FLTL.SLPTT.WRLO.FSC.IDQ.POS.MNM.,.fault.low angle.thrust slip.older over younger.thrust.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F197,.FLTV.SLPT.FMC.EXC.OBS.MEE.,.fault.variable angle.thrust slip.faulted metamorphic contact.existence certain.observable.location meets map accuracy standard.
,F198,.FLTV.SLPT.FMC.EXC.OBS.MNM.,.fault.variable angle.thrust slip.faulted metamorphic contact.existence certain.observable.location may not meet map accuracy standard.
,F199,.FLTV.SLPT.FMC.EXC.OBS.MNM.,.fault.variable angle.thrust slip.faulted metamorphic contact.existence certain.inferred.location may not meet map accuracy standard.
,F200,.FLTV.SLPT.FMC.INFM.MNM.,.fault.variable angle.thrust slip.faulted metamorphic contact.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F201,.FLTV.SLPT.FMC.INFU.MNM.,.fault.variable angle.thrust slip.faulted metamorphic contact.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F202,.FLTV.SLPT.FMC.EXQ.INF.MNM.,.fault.variable angle.thrust slip.faulted metamorphic contact.existence questionable.inferred.location may not meet map accuracy standard.
,F203,.FLTV.SLPT.FMC.EXQ.INFM.MNM.,.fault.variable angle.thrust slip.faulted metamorphic contact.existence questionable.Inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F204,.FLTV.SLPT.FMC.EXQ.INFU.MNM.,.fault.variable angle.thrust slip.faulted metamorphic contact.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F205,.FLTV.SLPNRS.EXC.OBS.MEE.,.fault.variable angle.rotational normal slip.slide fault.existence certain.observable.location may not meet map accuracy standard.
,F207,.FLTV.SLPNRS.EXC.INF.MNM.,.fault.variable angle.rotational normal slip.slide fault.existence certain.inferred.location may not meet map accuracy standard.
,F208,.FLTV.SLPNRS.EXC.INFM.MNM.,.fault.variable angle.rotational normal slip.slide fault.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F209,.FLT.SLPNRS.EXC.INFU.MNM.,.fault.variable angle.rotational normal slip.slide fault.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F210N,.FLTV.SLPNRS.INF.EXQ.MNM.,.fault.variable angle.rotational normal slip.slide fault.existence questionable.inferred.location may not meet map accuracy standard.
,F211N,.FLT.SLPNRS.EXQ.INFM.MNM.,.fault.variable angle.rotational normal slip.slide fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F212N,.FLT.SLPNRS.EXQ.INFU.MNM.,.fault.variable angle.rotational normal slip.slide fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F213,.FLTD.GPH.GPHA.MNM.,.fault.inferred by indirect methods.geophysics.aeromagnetic survey.location may not meet map accuracy standard.
,F214,.FLTD.GPH.GPHM.MNM.,.fault.inferred by indirect methods.geophysics.ground magnetic survey.location may not meet map accuracy standard.
,F215,.FLTD.GPH.GPHG.MNM.,.fault.inferred by indirect methods.geophysics.gravity survey.location may not meet map accuracy standard.
,F216,.FLTD.GPH.GPHR.MNM.,.fault.inferred by indirect methods.geophysics.radiometric survey.location may not meet map accuracy standard.
,F217,.FLTD.RSI.MNM.,.fault.inferred by indirect methods.remote-sensing imagery.location may not meet map accuracy standard.
,F218,.FLTD.GWL.MNM.,.fault.inferred by indirect methods.ground water levels.location may not meet map accuracy standard.
,F219,.FLTD.SSB.MNM.,.fault.inferred by indirect methods.subsurface boring data.location may not meet map accuracy standard.
,F220,.FLTI.,.fault.intruded
,GF1,.GEOE.IDC.OBS.LOW.,.geomorphic feature.eolian sand dune crest.identity certain.observable.located well but may not meet map accuracy standard.
,GF2,.GEOP.IDC.OBS.LOW.,.geomorphic feature.sag pond outline.identity certain.observable.located well but may not meet map accuracy standard.
,GF3,.GEOG.IDC.OBS.LOW.,.geomorphic feature.glacial moraine crest.identity certain.observable.located well but may not meet map accuracy standard.
,GF4,.GEODC.IDC.OBS.LOW.,.geomorphic feature.debris flow crest.identity certain.observable.located well but may not meet map accuracy standard.
,GF5,.GEODO.IDC.OBS.LOW.,.geomorphic feature.debris flow outline.identity certain.observable.located well but may not meet map accuracy standard.
,GF6,.GEOLC.IDC.OBS.LOW.,.geomorphic feature.landslide debris train crest.identity certain.observable.located well but may not meet map accuracy standard.
,GF7,.GEOTU.IDC.OBS.LOW.,.geomorphic feature.topographic scarp origin unknown.identity certain.observable.located well but may not meet map accuracy standard.
,GF8,.GEOLD.IDC.OBS.LOW.,.geomorphic feature.landslide closed depression.identity certain.observable.located well but may not meet map accuracy standard.
,GF9,.GEOTG.IDC.OBS.LOW.,.geomorphic feature.ground-failure crown scarp.identity certain.observable.located well but may not meet map accuracy standard.
,GF10,.GEOS.IDC.OBS.LOW.,.geomorphic feature.lakeshore strand line.identity certain.observable.located well but may not meet map accuracy standard.
,GF11,.GEOS.IDC.OBS.LOW.,.geomorphic feature.lakeshore strand line.identity certain.observable.located well but may not meet map accuracy standard.
,GF12,.GEOS.IDC.OBS.LOW.,.geomorphic feature.lakeshore strand line.identity certain.observable.located well but may not meet map accuracy standard.
,FZ1,.FZBSG.,.fault zone boundary.scratch.generic.
,FZ2,.FZBSB.,.fault zone boundary.scratch.boundary of fault breccia zone.
,FZ3,.FZBSC.,.fault zone boundary.scratch.boundary of cataclastic zone.
,FZ4,.FZBSM.,.fault zone boundary.scratch.boundary of mylonite zone.
,FA1,.FAXNA.UPR.SHZ.EXC.OBS.MEE.,.fold axial trace.fold form not determined.antiform.upright.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA2,.FAXNA.UPR.SHZ.EXC.OBS.MNM.,.fold axial trace.fold form not determined.antiform.upright.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA3,.FAXNA.UPR.SHZ.EXC.INF.MNM.,.fold axial trace.fold form not determined.antiform.upright.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA4,.FAXNA.UPR.SHZ.EXC.INFM.MNM.,.fold axial trace.fold form not determined.antiform.upright.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA5,.FAXNA.UPR.SHZ.EXC.INFU.MNM.,.fold axial trace.fold form not determined.antiform.upright.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA6,.FAXNA.UPR.SHZ.EXQ.INF.MNM.,.fold axial trace.fold form not determined.antiform.upright.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA7,.FAXNA.UPR.SHZ.EXQ.INFM.MNM.,.fold axial trace.fold form not determined.antiform.upright.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA8,.FAXNA.UPR.SHZ.EXQ.INFU.MNM.,.fold axial trace.fold form not determined.antiform.upright.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA9,.FAXNA.UPR.PLG.EXC.OBS.MEE.,.fold axial trace.fold form not determined.antiform.upright.plunging.existence certain.observable.location meets map accuracy standard.
,FA10,.FAXNA.UPR.PLG.EXC.OBS.MNM.,.fold axial trace.fold form not determined.antiform.upright.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA11,.FAXNA.UPR.PLG.EXC.INF.MNM.,.fold axial trace.fold form not determined.antiform.upright.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA12,.FAXNA.UPR.PLG.EXC.INFM.MNM.,.fold axial trace.fold form not determined.antiform.upright.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA13,.FAXNA.UPR.PLG.EXC.INFU.MNM.,.fold axial trace.fold form not determined.antiform.upright.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA14,.FAXNA.UPR.PLG.EXQ.INF.MNM.,.fold axial trace.fold form not determined.antiform.upright.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA15,.FAXNA.UPR.PLG.EXQ.INFM.MNM.,.fold axial trace.fold form not determined.antiform.upright.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA16,.FAXNA.UPR.PLG.EXQ.INFU.MNM.,.fold axial trace.fold form not determined.antiform.upright.plunging.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA17,.FAXNA.OVT.SHZ.EXC.OBS.MEE.,.fold axial trace.fold form not determined.antiform.overturned.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA18,.FAXNA.OVT.SHZ.EXC.OBS.MNM.,.fold axial trace.fold form not determined.antiform.overturned.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA19,.FAXNA.OVT.SHZ.EXC.INF.MNM.,.fold axial trace.fold form not determined.antiform.overturned.subhorizontal.existence certain.location may not meet map accuracy standard.
,FA20,.FAXNA.OVT.SHZ.EXC.INFM.MNM.,.fold axial trace.fold form not determined.antiform.overturned.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA21,.FAXNA.OVT.SHZ.EXC.INFU.MNM.,.fold axial trace.fold form not determined.antiform.overturned.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA22,.FAXNA.OVT.SHZ.EXQ.INF.MNM.,.fold axial trace.fold form not determined.antiform.overturned.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA23,.FAXNA.OVT.SHZ.EXQ.INFM.MNM.,.fold axial trace.fold form not determined.antiform.overturned.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA24,.FAXNA.OVT.SHZ.EXQ.INFU.MNM.,.fold axial trace.fold form not determined.antiform.overturned.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA25,.FAXNA.OVT.PLG.EXC.OBS.MEE.,.fold axial trace.fold form not determined.antiform.overturned.plunging.existence certain.observable.location meets map accuracy standard.
,FA26,.FAXNA.OVT.PLG.EXC.OBS.MNM.,.fold axial trace.fold form not determined.antiform.overturned.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA27,.FAXNA.OVT.PLG.EXC.INF.MNM.,.fold axial trace.fold form not determined.antiform.overturned.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA28,.FAXNA.OVT.PLG.EXC.INFM.MNM.,.fold axial trace.fold form not determined.antiform.overturned.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA29,.FAXNA.OVT.PLG.EXC.INFU.MNM.,.fold axial trace.fold form not determined.antiform.overturned.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA30,.FAXNA.OVT.PLG.EXQ.INF.MNM.,.fold axial trace.fold form not determined.antiform.overturned.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA31,.FAXNA.OVT.PLG.EXQ.INFM.MNM.,.fold axial trace.fold form not determined.antiform.overturned.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA32,.FAXNA.OVT.PLG.EXQ.INFU.MNM.,.fold axial trace.fold form not determined.antiform.overturned.plunging.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA33,.FAXDA.UPR.SHZ.EXC.OBS.MEE.,.fold axial trace.fold form determined.anticline.upright.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA34,.FAXDA.UPR.SHZ.EXC.OBS.MNM.,.fold axial trace.fold form determined.anticline.upright.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA35,.FAXDA.UPR.SHZ.EXC.INF.MNM.,.fold axial trace.fold form determined.anticline.upright.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA36,.FAXDA.UPR.SHZ.EXC.INFM.MNM.,.fold axial trace.fold form determined.anticline.upright.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA37,.FAXDA.UPR.SHZ.EXC.INFU.MNM.,.fold axial trace.fold form determined.anticline.upright.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA38,.FAXDA.UPR.SHZ.EXQ.INF.MNM.,.fold axial trace.fold form determined.anticline.upright.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA39,.FAXDA.UPR.SHZ.EXQ.INFM.MNM.,.fold axial trace.fold form determined.anticline.upright.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA40,.FAXDA.UPR.SHZ.EXQ.INFU.MNM.,.fold axial trace.fold form determined.anticline.upright.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA41,.FAXDA.UPR.PLG.EXC.OBS.MEE.,.fold axial trace.fold form determined.anticline.upright.plunging.existence certain.observable.location meets map accuracy standard.
,FA42,.FAXDA.UPR.PLG.EXC.OBS.MNM.,.fold axial trace.fold form determined.anticline.upright.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA43,.FAXDA.UPR.PLG.EXC.INF.MNM.,.fold axial trace.fold form determined.anticline.upright.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA44,.FAXDA.UPR.PLG.EXC.INFM.MNM.,.fold axial trace.fold form determined.anticline.upright.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA45,.FAXDA.UPR.PLG.EXC.INFU.MNM.,.fold axial trace.fold form determined.anticline.upright.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA46,.FAXDA.UPR.PLG.EXQ.INF.MNM.,.fold axial trace.fold form determined.anticline.upright.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA47,.FAXDA.UPR.PLG.EXQ.INFM.MNM.,.fold axial trace.fold form determined.anticline.upright.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA48,.FAXDA.UPR.PLG.EXQ.INFU.MNM.,.fold axial trace.fold form determined.anticline.upright.plunging.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA49,.FAXDA.OVT.SHZ.EXC.OBS.MEE.,.fold axial trace.fold form determined.anticline.overturned.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA50,.FAXDA.OVT.SHZ.EXC.OBS.MNM.,.fold axial trace.fold form determined.anticline.overturned.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA51,.FAXDA.OVT.SHZ.EXC.INF.MNM.,.fold axial trace.fold form determined.anticline.overturned.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA52,.FAXDA.OVT.SHZ.EXC.INFM.MNM.,.fold axial trace.fold form determined.anticline.overturned.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA53,(.FAXDA.OVT.SHZ.EXC.INFU.MNM.,.fold axial trace.fold form determined.anticline.overturned.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA54,.FAXDA.OVT.SHZ.EXQ.INF.MNM.,.fold axial trace.fold form determined.anticline.overturned.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA55,.FAXDA.OVT.SHZ.EXQ.INFM.MNM.,.fold axial trace.fold form determined.anticline.overturned.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA56,.FAXDA.OVT.SHZ.EXQ.INFU.MNM.,.fold axial trace.fold form determined.anticline.overturned.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA57,.FAXDA.OVT.PLG.EXC.OBS.MEE.,.fold axial trace.fold form determined.anticline.overturned.plunging.existence certain.observable.location meets map accuracy standard.
,FA58,.FAXDA.OVT.PLG.EXC.OBS.MNM.,.fold axial trace.fold form determined.anticline.overturned.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA59,.FAXDA.OVT.PLG.EXC.INF.MNM.,.fold axial trace.fold form determined.anticline.overturned.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA60,.FAXDA.OVT.PLG.EXC.INFM.MNM.,.fold axial trace.fold form determined.anticline.overturned.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA61,.FAXDA.OVT.PLG.EXC.INFU.MNM.,.fold axial trace.fold form determined.anticline.overturned.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA62,.FAXDA.OVT.PLG.EXQ.INF.MNM.,.fold axial trace.fold form determined.anticline.overturned.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA63,.FAXDA.OVT.PLG.EXQ.INFM.MNM.,.fold axial trace.fold form determined.anticline.overturned.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA64,.FAXDA.OVT.PLG.EXQ.INFU.MNM.,.fold axial trace.fold form determined.anticline.overturned.plunging.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA65,.FAXNS.UPR.SHZ.EXC.OBS.MEE.,.fold axial trace.fold form not determined.synform.upright.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA66,.FAXNS.UPR.SHZ.EXC.OBS.MNM.,.fold axial trace.fold form not determined.synform.upright.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA67,.FAXNS.UPR.SHZ.EXC.INF.MNM.,.fold axial trace.fold form not determined.synform.upright.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA68,.FAXNS.UPR.SHZ.EXC.INFM.MNM.,.fold axial trace.fold form not determined.synform.upright.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA69,.FAXNS.UPR.SHZ.EXC.INFU.MNM.,.fold axial trace.fold form not determined.synform.upright.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA70,.FAXNS.UPR.SHZ.EXQ.INF.MNM.,.fold axial trace.fold form not determined.synform.upright.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA71,.FAXNS.UPR.SHZ.EXQ.INFM.MNM.,.fold axial trace.fold form not determined.synform.upright.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA72,.FAXNS.UPR.SHZ.EXQ.INFU.MNM.,.fold axial trace.fold form not determined.synform.upright.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA73,.FAXNS.UPR.PLG.EXC.OBS.MEE.,.fold axial trace.fold form not determined.synform.upright.plunging.existence certain.observable.location meets map accuracy standard.
,FA74,.FAXNS.UPR.PLG.EXC.OBS.MNM.,.fold axial trace.fold form not determined.synform.upright.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA75,.FAXNS.UPR.PLG.EXC.INF.MNM.,.fold axial trace.fold form not determined.synform.upright.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA76,.FAXNS.UPR.PLG.EXC.INFM.MNM.,.fold axial trace.fold form not determined.synform.upright.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA77,.FAXNS.UPR.PLG.EXC.INFU.MNM.,.fold axial trace.fold form not determined.synform.upright.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA78,.FAXNS.UPR.PLG.EXQ.INF.MNM.,.fold axial trace.fold form not determined.synform.upright.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA79,.FAXNS.UPR.PLG.EXQ.INFM.MNM.,.fold axial trace.fold form not determined.synform.upright.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA80,.FAXNS.UPR.PLG.EXQ.INFU.MNM.,.fold axial trace.fold form not determined.synform.upright.plunging.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA81,.FAXNS.OVT.SHZ.EXC.OBS.MEE.,.fold axial trace.fold form not determined.synform.overturned.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA82,.FAXNS.OVT.SHZ.EXC.OBS.MNM.,.fold axial trace.fold form not determined.synform.overturned.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA83,.FAXNS.OVT.SHZ.EXC.INF.MNM.,.fold axial trace.fold form not determined.synform.overturned.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA84,.FAXNS.OVT.SHZ.EXC.INFM.MNM.,.fold axial trace.fold form not determined.synform.overturned.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA85,.FAXNS.OVT.SHZ.EXC.INFU.MNM.,.fold axial trace.fold form not determined.synform.overturned.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA86,.FAXNS.OVT.SHZ.EXQ.INF.MNM.,.fold axial trace.fold form not determined.synform.overturned.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA87,.FAXNS.OVT.SHZ.EXQ.INFM.MNM.,.fold axial trace.fold form not determined.synform.overturned.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA88,.FAXNS.OVT.SHZ.EXQ.INFU.MNM.,.fold axial trace.fold form not determined.synform.overturned.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA89,.FAXNS.OVT.PLG.EXC.OBS.MEE.,.fold axial trace.fold form not determined.synform.overturned.plunging.existence certain.observable.location meets map accuracy standard.
,FA90,.FAXNS.OVT.PLG.EXC.OBS.MNM.,.fold axial trace.fold form not determined.synform.overturned.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA91,.FAXNS.OVT.PLG.EXC.INF.MNM.,.fold axial trace.fold form not determined.synform.overturned.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA92,.FAXNS.OVT.PLG.EXC.INFM.MNM.,.fold axial trace.fold form not determined.synform.overturned.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA93,.FAXNS.OVT.PLG.EXC.INFU.MNM.,.fold axial trace.fold form not determined.synform.overturned.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA94,.FAXNS.OVT.PLG.EXQ.INF.MNM.,.fold axial trace.fold form not determined.synform.overturned.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA95,.FAXNS.OVT.PLG.EXQ.INFM.MNM.,.fold axial trace.fold form not determined.synform.overturned.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA96,.FAXNS.OVT.PLG.EXQ.INFU.MNM.,.fold axial trace.fold form not determined.synform.overturned.plunging.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA97,.FAXDS.UPR.SHZ.EXC.OBS.MEE.,.fold axial trace.fold form determined.syncline.upright.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA98,.FAXDS.UPR.SHZ.EXC.OBS.MNM.,.fold axial trace.fold form determined.syncline.upright.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA99,.FAXDS.UPR.SHZ.EXC.INF.MNM.,.fold axial trace.fold form determined.syncline.upright.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA100,.FAXDS.UPR.SHZ.EXC.INFM.MNM.,.fold axial trace.fold form determined.syncline.upright.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA101,.FAXDS.UPR.SHZ.EXC.INFU.MNM.,.fold axial trace.fold form determined.syncline.upright.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA102,.FAXDS.UPR.SHZ.EXQ.INF.MNM.,.fold axial trace.fold form determined.syncline.upright.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA103,.FAXDS.UPR.SHZ.EXQ.INFM.MNM.,.fold axial trace.fold form determined.syncline.upright.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA104,.FAXDS.UPR.SHZ.EXQ.INFU.MNM.,.fold axial trace.fold form determined.syncline.upright.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA105,.FAXDS.UPR.PLG.EXC.OBS.MEE.,.fold axial trace.fold form determined.syncline.upright.plunging.existence certain.observable.location meets map accuracy standard.
,FA106,.FAXDS.UPR.PLG.EXC.OBS.MNM.,.fold axial trace.fold form determined.syncline.upright.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA107,.FAXDS.UPR.PLG.EXC.INF.MNM.,.fold axial trace.fold form determined.syncline.upright.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA108,.FAXDS.UPR.PLG.EXC.INFM.MNM.,.fold axial trace.fold form determined.syncline.upright.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA109,.FAXDS.UPR.PLG.EXC.INFU.MNM.,.fold axial trace.fold form determined.syncline.upright.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA110,.FAXDS.UPR.PLG.EXQ.INF.MNM.,.fold axial trace.fold form determined.syncline.upright.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA111,.FAXDS.UPR.PLG.EXQ.INFM.MNM.,.fold axial trace.fold form determined.syncline.upright.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA112,.FAXDS.UPR.PLG.EXQ.INFU.MNM.,.fold axial trace.fold form determined.syncline.upright.plunging.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA113,.FAXDS.OVT.SHZ.EXC.OBS.MEE.,.fold axial trace.fold form determined.syncline.overturned.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA114,.FAXDS.OVT.SHZ.EXC.OBS.MNM.,.fold axial trace.fold form determined.syncline.overturned.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA115,.FAXDS.OVT.SHZ.EXC.INF.MNM.,.fold axial trace.fold form determined.syncline.overturned.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA116,.FAXDS.OVT.SHZ.EXC.INFM.MNM.,.fold axial trace.fold form determined.syncline.overturned.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA117,.FAXDS.OVT.SHZ.EXC.INFU.MNM.,.fold axial trace.fold form determined.syncline.overturned.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA118,.FAXDS.OVT.SHZ.EXQ.INF.MNM.,.fold axial trace.fold form determined.syncline.overturned.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA119,.FAXDS.OVT.SHZ.EXQ.INFM.MNM.,.fold axial trace.fold form determined.syncline.overturned.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA120,.FAXDS.OVT.SHZ.EXQ.INFU.MNM.,.fold axial trace.fold form determined.syncline.overturned.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA121,.FAXDS.OVT.PLG.EXC.OBS.MEE.,.fold axial trace.fold form determined.syncline.overturned.plunging.existence certain.observable.location meets map accuracy standard.
,FA122,.FAXDS.OVT.PLG.EXC.OBS.MNM.,.fold axial trace.fold form determined.syncline.overturned.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA123,.FAXDS.OVT.PLG.EXC.INF.MNM.,.fold axial trace.fold form determined.syncline.overturned.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA124,.FAXDS.OVT.PLG.EXC.INFM.MNM.,.fold axial trace.fold form determined.syncline.overturned.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA125,.FAXDS.OVT.PLG.EXC.INFU.MNM.,.fold axial trace.fold form determined.syncline.overturned.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA126,.FAXDS.OVT.PLG.EXQ.INF.MNM.,.fold axial trace.fold form determined.syncline.overturned.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA127,.FAXDS.OVT.PLG.EXQ.INFM.MNM.,.fold axial trace.fold form determined.syncline.overturned.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA128,.FAXDS.OVT.PLG.EXQ.INFU.MNM.,.fold axial trace.fold form determined.syncline.overturned.plunging.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA129,.FAXRN.UPR.SHZ.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA130,.FAXRN.UPR.SHZ.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA131,.FAXRN.UPR.SHZ.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA132,.FAXRN.UPR.SHZ.EXC.INFM.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA133,.FAXRN.UPR.SHZ.EXC.INFU.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA134,.FAXRN.UPR.SHZ.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA135,.FAXRN.UPR.SHZ.EXQ.INFM.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA136,.FAXRN.UPR.SHZ.EXQ.INFU.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA137,.FAXRN.UPR.PLG.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form not determined.upright.plunging.existence certain.observable.location meets map accuracy standard.
,FA138,.FAXRN.UPR.PLG.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA139,.FAXRN.UPR.PLG.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA140,.FAXRN.UPR.PLG.EXC.INFM.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA141,.FAXRN.UPR.PLG.EXC.INFU.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA142,.FAXRN.UPR.PLG.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA143,.FAXRN.UPR.PLG.EXQ.INFM.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA144,.FAXRN.UPR.P.EQL.INFU.MNM.,.fold axial trace.refolded fold.fold form not determined.upright.plunging.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA145,.FAXRN.OVT.SHZ.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA146,.FAXRN.OVT.SHZ.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA147,.FAXRN.OVT.SHZ.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form no determined.overturned.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA148,.FAXRN.OVT.SHZ.EXC.INFM.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.subhorizontal.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA149,.FAXRN.OVT.SHZ.EXC.INFU.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.subhorizontal.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA150,.FAXRN.OVT.SHZ.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA151,.FAXRN.OVT.SHZ.EXQ.INFM.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.subhorizontal.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA152,.FAXRN.OVT.SHZ.EXQ.INFU.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.subhorizontal.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA153,.FAXRN.OVT.PLG.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form not determined.overturned.plunging.existence certain.observable.location meets map accuracy standard.
,FA154,.FAXRN.UPR.PLG.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA155,.FAXRN.UPR.PLG.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA156,.FAXRN.UPR.PLG.EXC.INFM.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.plunging.existence certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA157,.FAXRN.UPR.PLG.EXC.INFU.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.plunging.existence certain.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA158,.FAXRN.UPR.PLG.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA159,.FAXRN.UPR.PLG.EXQ.INFM.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.plunging.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,FA160,.FAXRN.UPR.PLG.EXQ.INFU.MNM.,.fold axial trace.refolded fold.fold form not determined.overturned.plunging.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,FA161,.FAXRDA.UPR.SHZ.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA162,.FAXRDA.UPR.SHZ.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA163,.FAXRDA.UPR.SHZ.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA164,.FAXRDA.UPR.SHZ.EXC.INFM.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.subhorizontal.existence certain.inferred beneath mapped covering unit.loc may not meet MAS.
,FA165,.FAXRDA.UPR.SHZ.EXC.INFU.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.subhorizontal.existence certain.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA166,.FAXRDA.UPR.SHZ.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.subhorizontal.existence questionable.inferred.loc may not meet MAS.
,FA167,.FAXRDA.UPR.SHZ.EXQ.INFM.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.subhorizontal.existence questionable.inferred beneath mapped covering unit.loc may not meet MAS.
,FA168,.FAXRDA.UPR.SHZ.EXQ.INFU.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.subhorizontal.existence questionable.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA169,.FAXRDA.UPR.PLG.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.plunging.existence certain.observable.location meets map accuracy standard.
,FA170,.FAXRDA.UPR.PLG.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA171,.FAXRDA.UPR.PLG.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA172,.FAXRDA.UPR.PLG.EXC.INFM.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.plunging.existence certain.inferred beneath mapped covering unit.loc may not meet MAS.
,FA173,.FAXRDA.UPR.PLG.EXC.INFU.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.plunging.existence certain.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA174,.FAXRDA.UPR.PLG.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA175,.FAXRDA.UPR.PLG.EXQ.INFM.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.plunging.existence questionable.inferred beneath mapped covering unit.loc may not meet MAS.
,FA176,.FAXRDA.UPR.PLG.EXQ.INFU.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).upright.plunging.existence questionable.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA177,.FAXRDA.OVT.SHZ.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA178,.FAXRDA.OVT.SHZ.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA179,.FAXRDA.OVT.SHZ.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA180,.FAXRDA.OVT.SHZ.EXC.INFM.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.subhorizontal.existence certain.inferred beneath mapped covering unit.loc may not meet MAS.
,FA181,.FAXRDA.OVT.SHZ.EXC.INFU.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.subhorizontal.existence certain.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA182,.FAXRDA.OVT.SHZ.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.subhorizontal.existence questionable.inferred.location may not meet map accuracy standard.
,FA183,.FAXRDA.OVT.SHZ.EXQ.INFM.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.subhorizontal.existence questionable.inferred beneath mapped covering unit.loc may not meet MAS.
,FA184,.FAXRDA.OVT.SHZ.EXQ.INFU.MNM.,.fold axial trace.refolded fold.form determined.antiformal syncline (inverted syncline).overturned.subhorizontal.existence questionable.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA185,.FAXRDA.OVT.PLG.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.plunging.existence certain.observable.location meets map accuracy standard.
,FA186,.FAXRDA.OVT.PLG.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA187,.FAXRDA.OVT.PLG.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA188,.FAXRDA.OVT.PLG.EXC.INFM.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.plunging.existence certain.inferred beneath mapped covering unit.loc may not meet MAS.
,FA189,.FAXRDA.OVT.PLG.EXC.INFU.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.plunging.existence certain.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA190,.FAXRN.FFD.FAXRDA.OVT.PLG.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form determined.antiformal syncline (inverted syncline).overturned.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA191,.FAXRN.FFD.FAXRDA.OVT.PLG.EXQ.INFM.MNM.,.fold axial trace.refolded fold.form determined.antiformal syncline (inverted syncline).overturned.plunging.existence questionable.inferred beneath mapped covering unit.loc may not meet MAS.
,FA192,.FAXRN.FFD.FAXRDA.OVT.PLG.EXQ.INFU.MNM.,.fold axial trace.refolded fold.form determined.antiformal syncline (inverted syncline).overturned.plunging.existence questionable.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA193,.FAXRDS.UPR.SHZ.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).upright.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA194,.FAXRDS.UPR.SHZ.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).upright.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA195,.FAXRDS.UPR.SHZ.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).upright.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA196,.FAXRDS.UPR.SHZ.EXC.INFM.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).upright.subhorizontal.existence certain.inferred beneath mapped covering unit.loc may not meet MAS.
,FA197,.FAXRDS.UPR.SHZ.EXC.INFU.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).upright.subhorizontal.existence certain.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA198,.FAXRDS.UPR.SHZ.EXQ.INF.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).upright.subhorizontal.existence questionable.inferred.loc may not meet MAS.
,FA199,.FAXRDS.UPR.SHZ.EXQ.INFM.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).upright.subhorizontal.existence questionable.inferred beneath mapped covering unit.loc may not meet MAS.
,FA200,.FAXRDS.UPR.SHZ.EXQ.INFU.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).upright.subhorizontal.existence questionable.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA201,.FAXRDS.UPR.PLG.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).upright.plunging.existence certain.observable.location meets map accuracy standard.
,FA202,.FAXRDS.UPR.PLG.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).upright.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA203,.FAXRDS.UPR.PLG.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).upright.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA204,.FAXRDS.UPR.PLG.EXC.INFM.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).upright.plunging.existence certain.inferred beneath mapped covering unit.loc may not meet MAS.
,FA205,.FAXRDS.UPR.PLG.EXC.INFU.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).upright.plunging.existence certain.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA206,.FAXRDS.UPR.PLG.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).upright.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA207,.FAXRDS.UPR.PLG.EXQ.INFM.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).upright.plunging.existence questionable.inferred beneath mapped covering unit.loc may not meet MAS.
,FA208,.FAXRDS.UPR.PLG.EXQ.INFU.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).upright.plunging.existence questionable.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA209,.FAXRDS.OVT.SHZ.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).overturned.subhorizontal.existence certain.observable.location meets map accuracy standard.
,FA210,.FAXRDS.OVT.SHZ.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).overturned.subhorizontal.existence certain.observable.location may not meet map accuracy standard.
,FA211,.FAXRDS.OVT.SHZ.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).overturned.subhorizontal.existence certain.inferred.location may not meet map accuracy standard.
,FA212,.FAXRDS.OVT.SHZ.EXC.INFM.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).overturned.subhorizontal.existence certain.inferred beneath mapped covering unit.loc may not meet MAS.
,FA213,.FAXRDS.OVT.SHZ.EXC.INFU.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).overturned.subhorizontal.existence certain.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA214,.FAXRDS.OVT.SHZ.EXQ.INF.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).overturned.subhorizontal.existence questionable.inferred.loc may not meet MAS.
,FA215,.FAXRDS.OVT.SHZ.EXQ.INFM.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).overturned.subhorizontal.existence questionable.inferred beneath mapped covering unit.loc may not meet MAS.
,FA216,.FAXRDS.OVT.SHZ.EXQ.INFU.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).overturned.subhorizontal.existence questionable.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA217,.FAXRDS.OVT.PLG.EXC.OBS.MEE.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).overturned.plunging.existence certain.observable.location meets map accuracy standard.
,FA218,.FAXRDS.OVT.PLG.EXC.OBS.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).overturned.plunging.existence certain.observable.location may not meet map accuracy standard.
,FA219,.FAXRDS.OVT.PLG.EXC.INF.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).overturned.plunging.existence certain.inferred.location may not meet map accuracy standard.
,FA220,.FAXRDS.OVT.PLG.EXC.INFM.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).overturned.plunging.existence certain.inferred beneath mapped covering unit.loc may not meet MAS.
,FA221,.FAXRDS.OVT.PLG.EXC.INFU.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).overturned.plunging.existence certain.inferred beneath unmapped covering unit.loc may not meet MAS.
,FA222,.FAXRDS.OVT.PLG.EXQ.INF.MNM.,.fold axial trace.refolded fold.fold form determined.synformal anticline (inverted anticline).overturned.plunging.existence questionable.inferred.location may not meet map accuracy standard.
,FA223,.FAXRDS.OVT.PLG.EXQ.INFM.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).overturned.plunging.existence questionable.inferred beneath mapped covering unit.loc may not meet MAS.
,FA224,.FAXRDS.OVT.PLG.EXQ.INFU.MNM.,.fold axial trace.refolded fold.form determined.synformal anticline (inverted anticline).overturned.plunging.existence questionable.inferred beneath unmapped covering unit.loc may not meet MAS.
,DK1,.DIK.IDC.OBS.LOW.,.dike.identity certain.observable.located well
,DK2,.DIK.IDC.INFM.MNM.,.dike.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,DK3,.DIK.IDQ.INF.MNM.,.dike.identity questionable.inferred.location may not meet map accuracy standard.
,DK4,.DIK.IDQ.INFM.MNM.,.dike.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,DK5,.DIK.IDC.OBS.LOW.,.dike.identity certain.observable.located well
,DK6,.DIK.IDC.INFM.MNM.,.dike.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,DK7,.DIK.IDQ.INF.MNM.,.dike.identity questionable.inferred.location may not meet map accuracy standard.
,DK8,.DIK.IDQ.INFM.MNM.,.dike.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,DK9,.DIK.IDC.OBS.MNM.,.dike.identity certain.observable.location may not meet map accuracy standard.
,DK10,.DIK.IDC.INFM.MNM.,.dike.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,DK11,.DIK.IDQ.INF.MNM.,.dike.identity questionable.inferred.location may not meet map accuracy standard.
,DK12,.DIK.IDQ.INFM.MNM.,.dike.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,VEN1,.VEN.IDC.OBS.LOW.,.vein.identity certain.observable.located well
,VEN2,.VEN.IDC.INFM.MNM.,.vein.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,VEN3,.VEN.IDQ.INF.MNM.,.vein.identity questionable.inferred.location may not meet map accuracy standard.
,VEN4,.VEN.IDQ.INFM.MNM.,.vein.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,VEN5,.VEN.IDC.OBS.LOW.,.vein.identity certain.observable.located well
,VEN6,.VEN.IDC.INFM.MNM.,.vein.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,VEN7,.VEN.IDQ.INF.MNM.,.vein.identity questionable.inferred.location may not meet map accuracy standard.
,VEN8,.VEN.IDQ.INFM.MNM.,.vein.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,VEN9,.VEN.IDC.OBS.MNM.,.vein.identity certain.observable.location may not meet map accuracy standard.
,VEN10,.VEN.IDC.INFM.MNM.,.vein.identity certain.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,VEN11,.VEN.IDQ.INF.MNM.,.vein.identity questionable.inferred.location may not meet map accuracy standard.
,VEN12,.VEN.IDQ.INFM.MNM.,.vein.identity questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,LT1,.LIN.LINF.IDC.OBS.LOW.,.lineament.fault line escarpment.identity certain.observable.located well but may not meet map accuracy standard.
,LT2,.LIN.LINA.IDC.OBS.LOW.,.lineament.aligned topographic saddles.identity certain.observable.located well but may not meet map accuracy standard.
,LT3,.LIN.LINB.IDC.OBS.LOW.,.lineament.base of fold controlled slope.identity certain.observable.located well but may not meet map accuracy standard.
,LT4,.LIN.LINE.IDC.OBS.LOW.,.lineament.eroded edge of resistant bed.identity certain.observable.located well but may not meet map accuracy standard.
,LT5,.LIN.LINU.IDC.OBS.LOW.,.lineament.origin unknown.identity certain.observable.located well but may not meet map accuracy standard.
,ML1,.MSC.TRNG.LOW.,.line of gravity transect.located well but may not meet map accuracy standard.
,ML2,.MSC.TRNM.LOW.,.line of magnetic transect.located well but may not meet map accuracy standard.
,ML3,.MSC.TRNR.LOW.,.line of radiometric transect.located well but may not meet map accuracy standard.
,ML4,.MSC.TRNS.LOW.,.line of seismic transect.located well but may not meet map accuracy standard.
,ML5,.MSC.MSS.LOW.,.line of measured stratigraphic section.located well but may not meet map accuracy standard.
,ML6,.MSC.GCS.LOW.,.line of geologic cross section.located well but may not meet map accuracy standard.
,ML7,.MSC.POLU.LOW.,.polygon boundary.geologic type and origin unknown.located well but may not meet map accuracy standard.
,C28R,.CON.CONL.CRW.IDQ.INF.MNM.,.landslide contact.crown scarp.identity questionable.location may not meet map accuracy standard.
,C40R,.CON.CONS.CONST.IDQ.INF.MNM.,.sedimentary contact.separates terraced alluvial units.identity questionable.inferred.location may not meet map accuracy standard.
,F61R,.FLTH.SLPUG.FSC.IDQ.PRO.MNM.,.high-angle fault.slip unspecified.generic fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F62R,.FLTH.SLPUG.FSC.IDQ.POS.MNM.,.high-angle fault.slip unspecified.generic fault.scarp.identity questionable.possible.location   may not meet map accuracy standard.
,F63R,.FLTH.SLPSR.FSC.IDQ.PRO.MNM.,.high-angle fault.strike slip.right lateral fault.scarp.identity questionable.probable.location may not meet map  accuracy standard.
,F64R,.FLTH.SLPSR.FSC.IDQ.POS.MNM.,.high-angle fault.strike slip.right lateral fault.scarp.identity questionable.possible.location  may not meet map accuracy standard.
,F65R,.FLTH.SLPSL.FSC.IDQ.PRO.MNM.,.high-angle fault.strike slip.left lateral fault.scarp.identity questionable.probable.location  may not meet map accuracy standard.
,F66R,.FLTH.SLPSL.FSC.IDQ.POS.MNM.,.high-angle fault.strike slip.left lateral fault.scarp.identity questionable.possible.location may not meet map  accuracy standard.
,F67R,.FLTH.SLPNN.FSC.IDQ.PRO.MNM.,.high-angle fault.normal slip.normal fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F68R,.FLTH.SLPNN.FSC.IDQ.POS.MNM.,.high-angle fault.normal slip.normal fault.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F69R,.FLTH.SLPRR.FSC.IDQ.PRO.MNM.,.high-angle fault.reverse slip.reverse fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F70R,.FLTH.SLPRR.FSC.IDQ.POS.MNM.,.high-angle fault.reverse slip.reverse fault.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F71R,.FLTH.SLPOO.FSC.IDQ.PRO.MNM.,.high-angle fault.oblique slip.oblique fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F71R,.FLTH.SLPOO.FSC.IDQ.PRO.MNM.,.high-angle fault.oblique slip.oblique fault.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F72R,.FLTH.SLPOO.FSC.IDQ.POS.MNM.,.high-angle fault.oblique slip.oblique fault.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F86R,.FLTL.SLPUL.WRLY.EXQ.INF.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence questionable.inferred.location  may not meet map accuracy standard.
,F87R,.FLTL.SLPUL.WRLY.EXQ.INFM.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F88R,.FLTL.SLPUL.WRLY.EXQ.INFU.MNM.,.fault.low angle.slip unspecified.younger over older.low angle fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F94R,.FLTL.SLPUL.WRLO.EXQ.INF.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence questionable.inferred.location may not meet map accuracy standard.
,F95R,.FLTL.SLPUL.WRLO.EXQ.INFM.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F96R,.FLTL.SLPUL.WRLO.EXQ.INFU.MNM.,.fault.low angle.slip unspecified.older over younger.low angle fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F102R,.FLTL.SLPNL.WRLY.EXQ.INF.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence questionable.inferred.location may not meet map accuracy standard.
,F103R,.FLTL.SLPNL.WRLY.EXQ.INFM.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F104R,.FLTL.SLPNL.WRLY.EXQ.INFU.MNM.,.fault.low angle.normal slip.younger over older.low angle normal fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F109R,.FLTL.SLPNDM.WRLO.EXQ.INF.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F110R,.FLTL.SLPNDM.WRLO.EXQ.INFM.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F111R,.FLTL.SLPNDM.WRLO.EXQ.INFU.MNM.,.fault.low angle.normal slip.younger over older.master detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F118R,.FLTL.SLPND.WRLY.EXQ.INF.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F119R,.FLTL.SLPND.WRLY.EXQ.INFM.MNM.,.fault.low angle.normal slip.younger over older.detachment.existence inferred.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F120R,.FLTL.SLPND.WRLY.EXQ.INFU.MNM.,.fault.low angle.normal slip.younger over older.detachment.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F126R,.FLTL.SLPNL.WRLY.EXQ.INF.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F127R,.FLTL.SLPNL.WRLY.EXQ.INFM.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F128R,.FLTL.SLPNL.WRLY.EXQ.INFU.MNM.,.fault.low angle.normal slip.younger over older.listric into detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F134N,.FLTL.SLPNDM.WRLO.EXQ.INF.MNM.,.fault.low angle.normal slip.older over younger.master detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F135N,.FLTL.SLPNDM.WRLO.EXQ.INFM.MNM.,.fault.low angle.normal slip.older over younger.master detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F136N,.FLTL.SLPNDM.WRLO.EXQ.INFU.MNM.,.fault.low angle.normal slip.older over younger.master detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F142N,.FLTL.SLPND.WRLO.EXQ.INF.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F143N,.FLTL.SLPND.WRLO.EXQ.INFM.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F144N,.FLTL.SLPND.WRLO.EXQ.INFU.MNM.,.fault.low angle.normal slip.older over younger.detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F150N,.FLTL.SLPNL.WRLO.EXQ.INF.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence questionable.inferred.location may not meet map accuracy standard.
,F151N,.FLTL.SLPNL.WRLO.EXQ.INFM.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F152N,.FLTL.SLPNL.WRLO.EXQ.INFU.MNM.,.fault.low angle.normal slip.older over younger.listric into detachment.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F158R,.FLTL.SLPTD.WRLY.EXQ.INF.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence questionable.inferred.location may not meet map accuracy standard.
,F159R,.FLTL.SLPTD.WRLY.EXQ.INFM.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F160R,.FLTL.SLPTD.WRLY.EXQ.INFU.MNM.,.fault.low angle.thrust slip.younger over older.decollement.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F166R,.FLTL.SLPTT.WRLY.EXQ.INF.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence questionable.inferred.location may not meet map accuracy standard.
,F167R,.FLTL.SLPTT.WRLY.EXQ.INFM.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F168R,.FLTL.SLPTT.WRLY.EXQ.INFU.MNM.,.fault.low angle.thrust slip.younger over older.thrust.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F174R,.FLTL.SLPTTO.WRLY.EXQ.INF.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence questionable.inferred.location may not meet map accuracy standard.
,F175R,.FLTL.SLPTTO.WRLY.EXQ.INFM.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F176R,.FLTL.SLPTTO.WRLY.EXQ.INFU.MNM.,.fault.low angle.thrust slip.younger over older.thrust.overturned.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F182R,.FLTL.SLPTT.WRLO.EXQ.INF.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence questionable.inferred.location may not meet map accuracy standard.
,F183R,.FLTL.SLPTT.WRLO.EXQ.INFM.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F184R,.FLTL.SLPTT.WRLO.EXQ.INFU.MNM.,.fault.low angle.thrust slip.older over younger.thrust.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F190R,.FLTL.SLPTTO.WRLO.EXQ.INF.MNM.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence questionable.inferred.location may not meet map accuracy standard.
,F191R,.FLTL.SLPTTO.WRLO.EXQ.INFM.MNM.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F192R,.FLTL.SLPTTO.WRLO.EXQ.INFU.MNM.,.fault.low angle.thrust slip.older over younger.thrust.overturned.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.
,F195R,.FLTL.SLPTT.WRLO.FSC.IDQ.PRO.MNM.,.fault.low angle.thrust slip.older over younger.thrust.scarp.identity questionable.probable.location may not meet map accuracy standard.
,F196R,.FLTL.SLPTT.WRLO.FSC.IDQ.POS.MNM.,.fault.low angle.thrust slip.older over younger.thrust.scarp.identity questionable.possible.location may not meet map accuracy standard.
,F210R,.FLTV.SLPNRS.EXQ.MNM.,.fault.variable angle.rotational normal slip.slide fault.existence questionable.inferred.location may not meet map accuracy standard.
,F211R,.FLT.SLPNRS.EXQ.INFM.MNM.,.fault.variable angle.rotational normal slip.slide fault.existence questionable.inferred beneath mapped covering unit.location may not meet map accuracy standard.
,F212R,.FLT.SLPNRS.EXQ.INFU.MNM.,.fault.variable angle.rotational normal slip.slide fault.existence questionable.inferred beneath unmapped covering unit.location may not meet map accuracy standard.